{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":20,"n_cols":6,"rows_kept":20,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAG-B / RXS-L"]
[]
[]
[]
[]
["","","","","FCAG50BVEB / RXS50L2V1B","FCAG60BVEB / RXS60L2V1B"]
["Kylkapacitet","Nom.","","kW","5.00","5.70"]
["Värmekapacitet","Nom.","","kW","6.00","7.00"]
["Nominell verkningsgrad","Årlig energiförbrukning","","kWh","705","820"]
["","COP","","","3.70","3.52"]
["","EER köldfaktor","","","3.55","3.48"]
["","Energimärkningsdirektiv","Kyla","","A","A"]
["","","Värme","","A","B"]
["Röranslutningar","Kondensvatten","YD","mm","VP25 (Ytterdiameter 32, innerdiameter 25)","VP25 (Ytterdiameter 32, innerdiameter 25)"]
["","Gas","YD","mm","12.70","12.70"]
["","Vätska","YD","mm","6.35","6.35"]
["Anm:","","","","(1) - Vid normaldrift: +22°C / + 32°C","(1) - Vid normaldrift: +22°C / + 32°C"]
["","","","","(2) - Nominella värmekapaciteter baseras på: inomhustemperatur: 20°CTT, utomhustemperatur: 7 °CTT, 6 °CVT, ekvivalent köldmedierörledning: 5m, nivåskillnad: 0 m.","(2) - Nominella värmekapaciteter baseras på: inomhustemperatur: 20°CTT, utomhustemperatur: 7 °CTT, 6 °CVT, ekvivalent köldmedierörledning: 5m, nivåskillnad: 0 m."]
["","","","","(3) - Se separat ritning för driftsområde","(3) - Se separat ritning för driftsområde"]
["","","","","(4) - Se separata ritningar för elektriska data","(4) - Se separata ritningar för elektriska data"]