{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":5,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCQ-C8 / RXS-F"]
[]
[]
[]
[]
["","","","","FCQ60C8VEB / RXS60F3V1B"]
["Kylkapacitet","Min.","","kW","0.9"]
["","Max.","","kW","6.0"]
["","Nom.","","kW","5.7 (1)"]
["Piping connections","Vätska","YD","mm","6.35"]
["","Gas","YD","mm","12.7"]
["","Drain","OD","mm","32"]
["Nominell verkningsgrad","Årlig energiförbrukning","","kWh","820"]
["","EER köldfaktor","","","3.48"]
["","COP","","","3.52"]
["","Energimärkningsdirektiv","Kyla","","A"]
["","","Värme","","B"]
["Värmekapacitet","Nom.","","kW","7.0 (2)"]
["","Min.","","kW","0.9"]
["","Max.","","kW","8.0"]
["Anm:","","","","(1) - Kyla: inomhustemperatur. 27 °CTT, 19,0 °CVT, utomhustemperatur. 35 °CTT; ekvivalent rörledningslängd: 5 m"]
["","","","","(2) - Värme: inomhustemperatur. 20 °CTT; utomhustemperatur 7°CTT, 6°CVT; ekvivalent köldmedierörledning: 5m"]
["","","","","(3) - Nominell verkningsgrad: kyla vid 35°/27° nominell last, värme vid 7°/20° nominell last"]