{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":7,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCQG-F / AZQS-BY1 UK"]
[]
[]
[]
[]
["","","","","FCQG100FVEB / AZQS100B7Y1B UK","FCQG125FVEB / AZQS125B7Y1B UK","FCQG140FVEB / AZQS140B7Y1B UK"]
["Kylkapacitet","Nom.","","kW","9.5","12.1","13.0"]
["Rumskyla","SEER","","","5.50"]
["","Årlig energiförbrukning","","kWh/a","605"]
["","Kapacitet","Pdesign","kW","9.50"]
["","Energieffektivitetsklass","","","A"]
["Rumsvärme (medelklimat)","Kapacitet","Pdesign","kW","7.60"]
["","SCOP/A","","","3.85"]
["","Energieffektivitetsklass","","","A"]
["","Årlig energiförbrukning","","kWh/a","2,764"]
["Nominell verkningsgrad","Årlig energiförbrukning","","kWh","1,480","1,952","2,313"]
["","EER köldfaktor","","","3.21","3.10","2.81"]
["","COP","","","3.50","3.41","3.30"]
["","Energimärkningsdirektiv","Kyla","","A","B"]
["","","Värme","","B","B"]
["Uppvärmningseffekt","Nom.","","kW","10.8","13.5","15.5"]
["Anm:","","","","(1) - Årlig energiförbruking enligt Energimärkningsdirektiv 2002/31/EC","(1) - Årlig energiförbruking enligt Energimärkningsdirektiv 2002/31/EC","(1) - Årlig energiförbruking enligt Energimärkningsdirektiv 2002/31/EC"]
["","","","","(2) - SEER och SCOP är enligt EN 14825","(2) - SEER och SCOP är enligt EN 14825","(2) - SEER och SCOP är enligt EN 14825"]
["","","","","(3) - Nominell verkningsgrad: kyla vid 35°/27° nominell last, värme vid 7°/20° nominell last","(3) - Nominell verkningsgrad: kyla vid 35°/27° nominell last, värme vid 7°/20° nominell last","(3) - Nominell verkningsgrad: kyla vid 35°/27° nominell last, värme vid 7°/20° nominell last"]