{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":29,"n_cols":22,"rows_kept":29,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCQG-F / RZQSG-LV1/LY1"]
[]
[]
[]
[]
["","","","","FCQG35FVEB / FCQG35FVEB / RZQSG71L2V1B","FCQG71FVEB / RZQSG71L2V1B","FCQG50FVEB / FCQG50FVEB / RZQSG100L7Y1B9","FCQG100FVEB / RZQSG100L7V1B","FCQG100FVEB / RZQSG100L7Y1B9","FCQG100FVEB / RZQSG100L7Y1B","FCQG35FVEB / FCQG35FVEB / FCQG35FVEB / RZQSG100L7V1B","FCQG35FVEB / FCQG35FVEB / FCQG35FVEB / RZQSG100L7Y1B9","FCQG50FVEB / FCQG50FVEB / RZQSG100L7V1B","FCQG50FVEB / FCQG50FVEB / FCQG50FVEB / RZQSG125L7V1B","FCQG60FVEB / FCQG60FVEB / RZQSG125L7Y1B9","FCQG125FVEB / RZQSG125L7V1B","FCQG125FVEB / RZQSG125L7Y1B9","FCQG125FVEB / RZQSG125L7Y1B","FCQG35FVEB / FCQG35FVEB / FCQG35FVEB / FCQG35FVEB / RZQSG125L7V1B","FCQG35FVEB / FCQG35FVEB / FCQG35FVEB / FCQG35FVEB / RZQSG125L7Y1B9","FCQG50FVEB / FCQG50FVEB / FCQG50FVEB / RZQSG125L7Y1B9","FCQG60FVEB / FCQG60FVEB / RZQSG125L7V1B"]
["Nedkylningskapacitet","Nom.","","kW","","6.8","","9.5","9.5","9.5 (3)","","","","","","12.0","12.0","12.0 (3)"]
["Rumskyla","SEER","","","4.30","5.11","4.30","5.11","5.11","5.11 (6)","4.30","4.30","4.30","4.30","4.30","5.11","5.11","5.11 (6)","4.00","4.00","4.30","4.30"]
["","Årlig energiförbrukning","","kWh/a","554","466","773.256","650.685","650.685","","773.256","773.256","773.256","976.744","976.744","821.918","821.918","","1,050","1,050","976.744","976.744"]
["","Kapacitet","Pdesign","kW","6.80","6.80","9.50","9.50","9.50","","9.50","9.50","9.50","12.00","12.00","12.00","12.00","","12.00","12.00","12.00","12.00"]
["","Energieffektivitetsklass","","","C","A","C","A","A","","C","C","C","C","C","A","A","","D","D","C","C"]
["Rumsvärme (medelklimat)","Kapacitet","Pdesign","kW","6.00","6.33","6.81","7.60","7.60","","6.81","6.81","6.81","8.03","8.03","8.03","8.03","","8.03","8.03","8.03","8.03"]
["","SCOP/A","","","3.40","3.81","3.40","3.80","3.80","3.80 (6)","3.40","3.40","3.40","3.40","3.40","3.81","3.81","3.81 (6)","3.40","3.40","3.40","3.40"]
["","Energieffektivitetsklass","","","A","A","A","A","A","","A","A","A","A","A","A","A","","A","A","A","A"]
["","Årlig energiförbrukning","","kWh/a","2,472","2,327","2,802","2,799","2,799","","2,802","2,802","2,802","3,305","3,306.471","2,949","2,949","","3,305","3,305","3,305","3,306.471"]
["Nominell verkningsgrad","Årlig energiförbrukning","","kWh","","971","","1,440","1,440","1,440","","","","","","1,870","1,870","1,870"]
["","EER köldfaktor","","","","3.21","","3.30","3.30","3.30","","","","","","3.21","3.21","3.21"]
["","COP","","","","3.61","","3.54","3.54","3.54","","","","","","3.41","3.41","3.41"]
["","Energimärkningsdirektiv","Kyla","","","A","","A","A","A","","","","","","A","A","A"]
["","","Värme","","","A","","B","B","A","","","","","","B","B","B"]
["Värmekapacitet","Nom.","","kW","","7.5","","10.8","10.8","10.8 (4)","","","","","","13.5","13.5","13.5 (4)"]
["Anm:","","","","(1) - EER/COP enligt Eurovent 2012, endast för användning utanför EU","","(1) - EER/COP enligt Eurovent 2012, endast för användning utanför EU","","","","(1) - EER/COP enligt Eurovent 2012, endast för användning utanför EU","(1) - EER/COP enligt Eurovent 2012, endast för användning utanför EU","(1) - EER/COP enligt Eurovent 2012, endast för användning utanför EU","(1) - EER/COP enligt Eurovent 2012, endast för användning utanför EU","(1) - EER/COP enligt Eurovent 2012, endast för användning utanför EU","","","","(1) - EER/COP enligt Eurovent 2012, endast för användning utanför EU","(1) - EER/COP enligt Eurovent 2012, endast för användning utanför EU","(1) - EER/COP enligt Eurovent 2012, endast för användning utanför EU","(1) - EER/COP enligt Eurovent 2012, endast för användning utanför EU"]
["","","","","","(1) - EER/COP enligt Eurovent 2012, endast för användning utanför EU","","(1) - EER/COP enligt Eurovent 2012, endast för användning utanför EU","(1) - EER/COP enligt Eurovent 2012, endast för användning utanför EU","(1) - Årlig energiförbrukning: baserat på en genomsnittlig användning av 500 driftstimmar per år vid full belastning (nominella förhållanden)","","","","","","(1) - EER/COP enligt Eurovent 2012, endast för användning utanför EU","(1) - EER/COP enligt Eurovent 2012, endast för användning utanför EU","(1) - Årlig energiförbrukning: baserat på en genomsnittlig användning av 500 driftstimmar per år vid full belastning (nominella förhållanden)"]
["","","","","","(2) - Nominell verkningsgrad: kyla vid 35°/27° nominell last, värme vid 7°/20° nominell last","","(2) - Nominell verkningsgrad: kyla vid 35°/27° nominell last, värme vid 7°/20° nominell last","(2) - Nominell verkningsgrad: kyla vid 35°/27° nominell last, värme vid 7°/20° nominell last","(2) - Energiklass: skala från A (mest effektiv) till G (mindre effektiv)","","","","","","(2) - Nominell verkningsgrad: kyla vid 35°/27° nominell last, värme vid 7°/20° nominell last","(2) - Nominell verkningsgrad: kyla vid 35°/27° nominell last, värme vid 7°/20° nominell last","(2) - Energiklass: skala från A (mest effektiv) till G (mindre effektiv)"]
["","","","","","","","","","(3) - Kyla: inomhustemperatur. 27 °CTT, 19 °CVT; utomhustemperatur 35 °CTT; ekvivalent rörledningslängd: 5 m, nivåskillnad: 0 m","","","","","","","","(3) - Kyla: inomhustemperatur. 27 °CTT, 19 °CVT; utomhustemperatur 35 °CTT; ekvivalent rörledningslängd: 5 m, nivåskillnad: 0 m"]
["","","","","","","","","","(4) - Värme: inomhustemperatur. 20 °CTT; utomhustemperatur 7°CTT, 6°CVT; ekvivalent köldmedierörledning: 5m, nivåskillnad: 0 m","","","","","","","","(4) - Värme: inomhustemperatur. 20 °CTT; utomhustemperatur 7°CTT, 6°CVT; ekvivalent köldmedierörledning: 5m, nivåskillnad: 0 m"]
["","","","","","","","","","(5) - Årlig energiförbruking enligt Energimärkningsdirektiv 2002/31/EC","","","","","","","","(5) - Årlig energiförbruking enligt Energimärkningsdirektiv 2002/31/EC"]
["","","","","","","","","","(6) - SEER och SCOP är enligt EN 14825","","","","","","","","(6) - SEER och SCOP är enligt EN 14825"]
["","","","","","","","","","(7) - Nominell verkningsgrad: kyla vid 35°/27° nominell last, värme vid 7°/20° nominell last","","","","","","","","(7) - Nominell verkningsgrad: kyla vid 35°/27° nominell last, värme vid 7°/20° nominell last"]