{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":8,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCQHG-F / RZQSG-L3/9V1"]
[]
[]
[]
[]
["","","","","FCQHG71FVEB / RZQSG71L3V1B","FCQHG100FVEB / RZQSG100L9V1B","FCQHG125FVEB / RZQSG125L9V1B","FCQHG140FVEB / RZQSG140L9V1B"]
["Kylkapacitet","Nom.","","kW","6.8","9.5","12.0","13.4"]
["Rumskyla","SEER","","","6.50","6.70","5.40"]
["","Årlig energiförbrukning","","kWh/a","366","497","778"]
["","Kapacitet","Pdesign","kW","6.80","9.50","12.00"]
["","Energieffektivitetsklass","","","A++","A++","A"]
["Rumsvärme (medelklimat)","Kapacitet","Pdesign","kW","7.60","8.03","8.03"]
["","SCOP/A","","","4.15","4.30","4.10"]
["","Energieffektivitetsklass","","","A+","A+","A+"]
["","Årlig energiförbrukning","","kWh/a","2,563","2,615","2,742"]
["Nominell verkningsgrad","Årlig energiförbrukning","","kWh","970","1,285","1,855"]
["","EER köldfaktor","","","3.50","3.70","3.23","3.21"]
["","COP","","","4.10","4.30","3.75","3.61"]
["","Energimärkningsdirektiv","Kyla","","A","A","A"]
["","","Värme","","A","A","A"]
["Uppvärmningseffekt","Nom.","","kW","7.5","10.8","13.5","15.5"]
["Anm:","","","","(1) - EER/COP enligt Eurovent 2012, endast för användning utanför EU","(1) - EER/COP enligt Eurovent 2012, endast för användning utanför EU","(1) - EER/COP enligt Eurovent 2012, endast för användning utanför EU","(1) - EER/COP enligt Eurovent 2012, endast för användning utanför EU"]
["","","","","(2) - Nominell verkningsgrad: kyla vid 35°/27° nominell last, värme vid 7°/20° nominell last","(2) - Nominell verkningsgrad: kyla vid 35°/27° nominell last, värme vid 7°/20° nominell last","(2) - Nominell verkningsgrad: kyla vid 35°/27° nominell last, värme vid 7°/20° nominell last","(2) - Nominell verkningsgrad: kyla vid 35°/27° nominell last, värme vid 7°/20° nominell last"]