{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":67,"n_cols":8,"rows_kept":67,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDA-A"]
[]
[]
[]
[]
["","","","","","FDA125A5VEB","FDA200AXVEB","FDA250AXVEB"]
["Kylkapacitet","Total kapacitet","","Nom.","kW","12.10","19.00","22.00"]
["Värmekapacitet","Total capacity","","Nom.","kW","13.50","22.4","24.0"]
["Hölje","Färg","","","","Omålat","Omålat","Omålat"]
["","Material","","","","Galvaniserat stål","Galvaniserad stålplåt","Galvaniserad stålplåt"]
["Mått","Enhet","","Höjd","mm","300","470","470"]
["","","","Bredd","mm","1,400","1,490","1,490"]
["","","","Djup","mm","700","1,100","1,100"]
["Vikt","Enhet","","","kg","45","104","115"]
["Ogiltig takhöjd >","mm","","","","350"]
["Fläkt","Luftflödeshastighet","Kyla","Hög","m³/min","39.0","64.0","69.0"]
["","","","Medium","m³/min","","50","56"]
["","","","Låg","m³/min","28.0","36.0","43.0"]
["","","Värme","Hög","m³/min","39.0","64.0","69.0"]
["","","","Medium","m³/min","","50.0","56.0"]
["","","","Låg","m³/min","28.0","36.0","43.0"]
["","Yttre statiskt tryck","","Hög","Pa","200","250","250"]
["","","","Nom.","Pa","50","62","62"]
["Sound power level","Kyla","","","dBA","66","69.0","71.0"]
["Ljudtrycksnivå","Kyla","","Hög","dBA","40","43.0","44.0"]
["","","","Medium","dBA","","39.0","40.0"]
["","","","Låg","dBA","33","36.0","37.0"]
["","Värme","","Hög","dBA","40","43.0","44.0"]
["","","","Medel","dBA","","39.0","40.0"]
["","","","Låg","dBA","33","36.0","37.0"]
["Röranslutningar","Vätska","","YD","mm","9.52","9.52","9.52"]
["","Gas","","YD","mm","15.90","19.1","22.2"]
["","Kondensvatten","","","","VP25 (I.D. 25/O.D. 32)","BSP1","BSP1"]
["Dräneringshöjd","mm","","","","625"]
["Dekorationspanel","Model","","","","BYBS125DJW1"]
["","Färg","","","","Vit (10Y9/0,5)"]
["","Dimensioner","","Höjd","mm","55"]
["","","","Bredd","mm","1,500"]
["","","","Djup","mm","500"]
["","Vikt","","","kg","6.5"]
["Styrsystem","Infrared remote control","","","","BRC4C65, BRC4C66"]
["","Wired remote control","","","","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52"]
["Standardtillbehör","Bruksanvisning","","","","","1","1"]
["","Installations- och bruksanvisning","","","","1","1","1"]
["","Installationsanvisning","","","","","1","1"]
["","Allmänna säkerhetsföreskrifter","","","","1","1","1"]
["","Gasanslutningsrör","","","","","1","1"]
["","Material kabelklämma","","","","","1","1"]
["","Bricka","","","","8","12","12"]
["","Fjäderbricka","","","","","2","2"]
["","Skruv + bricka","","","","","45","45"]
["","Hexagonshuvudskruv med bricka","","","","","49","49"]
["","Skruvar","","","","16","2","2"]
["","Hexagonshuvudskruv","","","","","2","2"]
["","Vanlig bricka","","","","","8","8"]
["Power supply","Namn","","","","","VE","VE"]
["","Fas","","","","1~","1~","1~"]
["","Frequency","","","Hz","50/60","50/60","50/60"]
["","Spänning","","","V","220-240/220","220-240/220","220-240/220"]
["Standardtillbehör","Slangband","","","","1"]
["","Kondensvattenslang","","","","1"]
["","Kablage för standard strömförsörjning","","","","2"]
["","Tätningsmaterial (dräneringsslang)","","","","1"]
["","Tätningsmaterial","","","","2"]
["","Termiskt isoleringsrör (vätska)","","","","1"]
["","Termiskt isoleringsrör (gas)","","","","1"]
["Anm:","","","","","(1) - Se separata ritningar för elektriska data"]