{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":22,"n_cols":5,"rows_kept":22,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDQ-B / RZQ-D3/D9V1"]
[]
[]
[]
[]
["","","","","FDQ125B8V3B9 / RZQ125D9V1B"]
["Kylkapacitet","Nom.","","kW","12.5 (3)"]
["Röranslutningar","Vätska","YD","mm","9.52"]
["","Gas","YD","mm","15.9"]
["","Kondensvatten","YD","mm","26"]
["Rumskyla","SEER","","","3.50"]
["Nominell verkningsgrad","Årlig energiförbrukning","","kWh","1,978"]
["","EER köldfaktor","","","3.16"]
["","COP","","","3.88"]
["","Energimärkningsdirektiv","Kyla","","B"]
["","","Värme","","A"]
["Värmekapacitet","Nom.","","kW","14.0 (4)"]
["Anm:","","","","(1) - Energiklass: skala från A (mest effektiv) till G (mindre effektiv)"]
["","","","","(2) - Årlig energiförbrukning: baserat på en genomsnittlig användning av 500 driftstimmar per år vid full belastning (nominella förhållanden)"]
["","","","","(3) - Kyla: inomhustemperatur. 27 °CTT, 19 °CVT; utomhustemperatur 35 °CTT; ekvivalent rörledningslängd: 5 m, nivåskillnad: 0 m"]
["","","","","(4) - Värme: inomhustemperatur. 20 °CTT; utomhustemperatur 7°CTT, 6°CVT; ekvivalent köldmedierörledning: 5m, nivåskillnad: 0 m"]
["","","","","(5) - Nominell verkningsgrad: kyla vid 35°/27° nominell last, värme vid 7°/20° nominell last"]