{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":28,"n_cols":7,"rows_kept":28,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDQ-C / RZQSG-LV1/LY1"]
[]
[]
[]
[]
["","","","","FDQ125C7VEB / RZQSG125L7V1B","FDQ125C7VEB / RZQSG125L7Y1B9","FDQ125C7VEB / RZQSG125L7Y1B"]
["Kylkapacitet","Nom.","","kW","12.0","12.0","12.0 (3)"]
["Rumskyla","SEER","","","4.35","4.35","4.35 (6)"]
["","Årlig energiförbrukning","","kWh/a","965.517","965.517"]
["","Kapacitet","Pdesign","kW","12.00","12.00"]
["","Energieffektivitetsklass","","","C","C"]
["Rumsvärme (medelklimat)","Kapacitet","Pdesign","kW","7.60","7.60"]
["","SCOP/A","","","3.81","3.81","3.81 (6)"]
["","Energieffektivitetsklass","","","A","A"]
["","Årlig energiförbrukning","","kWh/a","2,791","2,791"]
["Nominell verkningsgrad","Årlig energiförbrukning","","kWh","1,870","1,600","1,870"]
["","EER köldfaktor","","","3.21","3.21","3.21"]
["","COP","","","3.51","3.51","3.51"]
["","Energimärkningsdirektiv","Kyla","","A","A","A"]
["","","Värme","","B","B","B"]
["Värmekapacitet","Nom.","","kW","13.5","13.5","13.5 (4)"]
["Anm:","","","","(1) - EER/COP enligt Eurovent 2012, endast för användning utanför EU","(1) - EER/COP enligt Eurovent 2012, endast för användning utanför EU","(1) - Årlig energiförbrukning: baserat på en genomsnittlig användning av 500 driftstimmar per år vid full belastning (nominella förhållanden)"]
["","","","","(2) - Nominell verkningsgrad: kyla vid 35°/27° nominell last, värme vid 7°/20° nominell last","(2) - Nominell verkningsgrad: kyla vid 35°/27° nominell last, värme vid 7°/20° nominell last","(2) - Energiklass: skala från A (mest effektiv) till G (mindre effektiv)"]
["","","","","","","(3) - Kyla: inomhustemperatur. 27 °CTT, 19 °CVT; utomhustemperatur 35 °CTT; ekvivalent rörledningslängd: 5 m, nivåskillnad: 0 m"]
["","","","","","","(4) - Värme: inomhustemperatur. 20 °CTT; utomhustemperatur 7°CTT, 6°CVT; ekvivalent köldmedierörledning: 5m, nivåskillnad: 0 m"]
["","","","","","","(5) - Årlig energiförbruking enligt Energimärkningsdirektiv 2002/31/EC"]
["","","","","","","(6) - SEER och SCOP är enligt EN 14825"]
["","","","","","","(7) - Nominell verkningsgrad: kyla vid 35°/27° nominell last, värme vid 7°/20° nominell last"]