{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":29,"n_cols":6,"rows_kept":29,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXM-F3 / RXM-N"]
[]
[]
[]
[]
["","","","","FDXM50F3V1B / RXM50N2V1B","FDXM60F3V1B / RXM60N2V1B"]
["Kylkapacitet","Min.","","kW","1.70","1.70"]
["","Max.","","kW","5.30","6.50"]
["","Nom.","","kW","5.00","6.00"]
["Rumskyla","Årlig energiförbrukning","","kWh/a","","378"]
["","Kapacitet","Pdesign","kW","","6.00"]
["Rumsvärme (medelklimat)","Kapacitet","Pdesign","kW","","4.60"]
["","Årlig energiförbrukning","","kWh/a","","1,693"]
["Nominell verkningsgrad","Årlig energiförbrukning","","kWh","816","1,024"]
["","EER köldfaktor","","","3.06","2.93"]
["","COP","","","3.10","3.21"]
["","Energimärkningsdirektiv","Kyla","","B","C"]
["","","Värme","","D","C"]
["Uppvärmningseffekt","Nom.","","kW","5.80","7.00"]
["","Min.","","kW","1.70","1.70"]
["","Max.","","kW","6.00","7.10"]
["Anm:","","","","(1) - Se separat ritning för driftsområde","(1) - Se separat ritning för driftsområde"]
["","","","","(2) - Se separata ritningar för elektriska data","(2) - Se separata ritningar för elektriska data"]
["","","","","(3) - Nominell kylkapacitet baseras på: inomhustemperatur: 27°CTT, 19°CVT, utomhustemperatur: 35 °CTT, ekvivalent köldmedierörledning: 5 m, nivåskillnad: 0 m.","(3) - Nominell kylkapacitet baseras på: inomhustemp.: 27°CTT, 19°CVT, utomhustemperatur: 35 °CTT, ekvivalent köldmedierörledning: 5 m, nivåskillnad: 0 m."]
["","","","","(4) - Nominella värmekapaciteter baseras på: inomhustemperatur: 20°CTT, utomhustemperatur: 7 °CTT, 6 °CVT, ekvivalent köldmedierörledning: 5m, nivåskillnad: 0 m.","(4) - Nominella värmekapaciteter baseras på: inomhustemperatur: 20°CTT, utomhustemperatur: 7 °CTT, 6 °CVT, ekvivalent köldmedierörledning: 5m, nivåskillnad: 0 m."]
["Rumskyla","Energieffektivitetsklass","","","","A"]
["","SEER","","","","5.56"]
["Rumsvärme (medelklimat)","Energieffektivitetsklass","","","","A"]
["","SCOP/A","","","","3.80"]