{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":28,"n_cols":6,"rows_kept":28,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXM-F3 / RXS-L"]
[]
[]
[]
[]
["","","","","FDXM50F3V1B / RXS50L2V1B","FDXM60F3V1B / RXS60L2V1B"]
["Nedkylningskapacitet","Nom.","","kW","5.00","6.00"]
["Rumskyla","SEER","","","5.72","5.51"]
["","Årlig energiförbrukning","","kWh/a","306","381"]
["","Kapacitet","Pdesign","kW","5.00","6.00"]
["","Energieffektivitetsklass","","","A+","A"]
["Rumsvärme (medelklimat)","Kapacitet","Pdesign","kW","4.00","4.60"]
["","SCOP/A","","","3.93","3.80"]
["","Energieffektivitetsklass","","","A","A"]
["","Årlig energiförbrukning","","kWh/a","1,425","1,693"]
["Piping connections","Vätska","YD","mm","6.35","6.35"]
["","Gas","YD","mm","12.70","12.70"]
["","Kondensvatten","OD","mm","VP20 (Ytterdiameter 26, Innerdiameter 20)","VP20 (Ytterdiameter 26, Innerdiameter 20)"]
["Nominell verkningsgrad","EER köldfaktor","","","3.03","2.91"]
["","Årlig energiförbrukning","","kWh","825","1,030"]
["","COP","","","3.10","3.21"]
["","Energimärkningsdirektiv","Kyla","","B","C"]
["","","Värme","","D","C"]
["Värmekapacitet","Nom.","","kW","5.80","7.00"]
["Anm:","","","","(1) - Nominell kylkapacitet baseras på: inomhustemperatur: 27°CTT, 19°CVT, utomhustemperatur: 35 °CTT, ekvivalent köldmedierörledning: 5 m, nivåskillnad: 0 m.","(1) - Nominell kylkapacitet baseras på: inomhustemperatur: 27°CTT, 19°CVT, utomhustemperatur: 35 °CTT, ekvivalent köldmedierörledning: 5 m, nivåskillnad: 0 m."]
["","","","","(2) - Nominella värmekapaciteter baseras på: inomhustemperatur: 20°CTT, utomhustemperatur: 7 °CTT, 6 °CVT, ekvivalent köldmedierörledning: 5m, nivåskillnad: 0 m.","(2) - Nominella värmekapaciteter baseras på: inomhustemperatur: 20°CTT, utomhustemperatur: 7 °CTT, 6 °CVT, ekvivalent köldmedierörledning: 5m, nivåskillnad: 0 m."]
["","","","","(3) - Se separat ritning för driftsområde","(3) - Se separat ritning för driftsområde"]
["","","","","(4) - Se separata ritningar för elektriska data","(4) - Se separata ritningar för elektriska data"]