{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":6,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXM-F9 / RXS-L3"]
[]
[]
[]
[]
["","","","","FDXM25F3V1B9 / RXS25L3V1B","FDXM35F3V1B9 / RXS35L3V1B"]
["Kylkapacitet","Min.","","kW","1.30","1.40"]
["","Max.","","kW","3.00","3.80"]
["","Nom.","","kW","2.40","3.40"]
["Röranslutningar","Vätska","YD","mm","6.35","6.35"]
["","Gas","YD","mm","9.50","9.50"]
["","Drain","OD","mm","VP20 (Ytterdiameter 26, Innerdiameter 20)","VP20 (Ytterdiameter 26, Innerdiameter 20)"]
["Nominell verkningsgrad","Årlig energiförbrukning","","kWh","321","574"]
["","EER köldfaktor","","","3.74","2.96"]
["","COP","","","4.00","3.48"]
["","Energimärkningsdirektiv","Kyla","","A","B"]
["","","Värme","","A","A"]
["Värmekapacitet","Nom.","","kW","3.20","4.00"]
["","Min.","","kW","1.30","1.40"]
["","Max.","","kW","4.50","5.00"]
["Anm:","","","","(1) - Nominell kylkapacitet baseras på: inomhustemperatur: 27°CTT, 19°CVT, utomhustemperatur: 35 °CTT, ekvivalent köldmedierörledning: 5 m, nivåskillnad: 0 m.","(1) - Nominell kylkapacitet baseras på: inomhustemperatur: 27°CTT, 19°CVT, utomhustemperatur: 35 °CTT, ekvivalent köldmedierörledning: 5 m, nivåskillnad: 0 m."]
["","","","","(2) - Nominella värmekapaciteter baseras på: inomhustemperatur: 20°CTT, utomhustemperatur: 7 °CTT, 6 °CVT, ekvivalent köldmedierörledning: 5m, nivåskillnad: 0 m.","(2) - Nominella värmekapaciteter baseras på: inomhustemperatur: 20°CTT, utomhustemperatur: 7 °CTT, 6 °CVT, ekvivalent köldmedierörledning: 5m, nivåskillnad: 0 m."]
["","","","","(3) - Se separat ritning för driftsområde","(3) - Se separat ritning för driftsområde"]
["","","","","(4) - Se separata ritningar för elektriska data","(4) - Se separata ritningar för elektriska data"]