{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":5,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXS-F9"]
[]
[]
[]
[]
["","","","","FDXS50F2VEB9"]
["Ljudtrycksnivå","Värme","Hög","dBA","38"]
["","","Medel","dBA","36"]
["","","Låg","dBA","30"]
["","Kyla","Medium","dBA","36"]
["","","Låg","dBA","30"]
["","","Hög","dBA","38"]
["Standardtillbehör","Installationsanvisning","","","1"]
["","Bruksanvisning","","","1"]
["","Isolering för anslutningsdel","","","1"]
["","Tätningsbelägg","","","1"]
["","Metall för rörhållare","","","1"]
["","Kondensvattenslang","","","1"]
["","Bricka för hängarfäste","","","8"]
["","Tätningsmaterial","","","2"]
["","Rörhållare","","","6"]
["","Brickhållarplåt","","","4"]
["","Skruvar för rörflänsar","","","1"]
["","Luftfilter","","","1"]
["Röranslutningar","Vätska","YD","mm","6.35"]
["","Gas","YD","mm","12.7"]
["","Kondensvatten","","","VP20 (I.D. 20/O.D. 26)"]
["Ineffekt","Kyla","Nom.","kW","0.060"]
["","Värme","Nom.","kW","0.060"]
["Ljudeffektsnivå","Kyla","","dBA","55"]
["","Värme","","dBA","55"]
["Mått","Enhet","Bredd","mm","1,150"]
["","","Djup","mm","620"]
["","","Höjd","mm","200"]
["Vikt","Enhet","","kg","30.0"]
["Fläkt","Yttre statiskt tryck","Nom.","Pa","40"]
["Power supply","Phase","","","1~"]
["","Frequency","","Hz","50/60"]
["","Namn","","","VE"]
["","Spänning","","V","220-240"]
["Anm:","","","","(1) - Vid anslutning till en utomhusdel med multisystem, se specifikationerna för multiutomhusdelen som ska anslutas."]