{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":42,"n_cols":8,"rows_kept":42,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FFA-A / RXM-M9"]
[]
[]
[]
[]
["","","","","FFA25A2VEB / RXM25M3V1B9","FFA35A2VEB / RXM35M3V1B9","FFA50A2VEB / RXM50M3V1B9","FFA60A2VEB / RXM60M3V1B9"]
["Kylkapacitet","Nom.","","kW","2.50","3.40"]
["Rumskyla","SEER","","","6.17","6.38"]
["","Årlig energiförbrukning","","kWh/a","142","186"]
["","Kapacitet","Pdesign","kW","2.50","3.40"]
["","Energieffektivitetsklass","","","A++","A++"]
["Rumsvärme (medelklimat)","Kapacitet","Pdesign","kW","2.31","3.10"]
["","SCOP/A","","","4.24","4.10"]
["","Energieffektivitetsklass","","","A+","A+"]
["","Årlig energiförbrukning","","kWh/a","762","1,058"]
["Nominell verkningsgrad","Årlig energiförbrukning","","kWh","273","446"]
["","EER köldfaktor","","","4.57","3.81"]
["","COP","","","3.90","3.50"]
["","Energimärkningsdirektiv","Kyla","","A","A"]
["","","Värme","","A","B"]
["Värmekapacitet","Nom.","","kW","3.20","4.20"]
["Anm:","","","","(1) - Se separata ritningar för elektriska data","(1) - Se separata ritningar för elektriska data"]
["","","","","(2) - Se separat ritning för driftsområde","(2) - Se separat ritning för driftsområde"]
["","","","","(3) - Nominell kylkapacitet baseras på: inomhustemp.: 27°CTT, 19°CVT, utomhustemperatur: 35 °CTT, ekvivalent köldmedierörledning: 5 m, nivåskillnad: 0 m.","(3) - Nominell kylkapacitet baseras på: inomhustemp.: 27°CTT, 19°CVT, utomhustemperatur: 35 °CTT, ekvivalent köldmedierörledning: 5 m, nivåskillnad: 0 m."]
["","","","","(4) - Nominella värmekapaciteter baseras på: inomhustemperatur: 20°CTT, utomhustemperatur: 7 °CTT, 6 °CVT, ekvivalent köldmedierörledning: 5m, nivåskillnad: 0 m.","(4) - Nominella värmekapaciteter baseras på: inomhustemperatur: 20°CTT, utomhustemperatur: 7 °CTT, 6 °CVT, ekvivalent köldmedierörledning: 5m, nivåskillnad: 0 m."]
["Outdoor unit","","","","","","RXM50M3V1B9","RXM60M3V1B9"]
["Kylkapacitet","Nom.","","kW","","","5.00","5.70"]
["Värmekapacitet","Nom.","","kW","","","5.80","7.00"]
["Nominell verkningsgrad","EER köldfaktor","","","","","3.24","3.05"]
["","COP","","","","","3.49","3.41"]
["","Årlig energiförbrukning","","kWh","","","771","934"]
["","Energimärkningsdirektiv","Kyla","","","","A","B"]
["","","Värme","","","","B","B"]
["Rumskyla","Energieffektivitetsklass","","","","","A+","A+"]
["","Kapacitet","Pdesign","kW","","","5.00","5.70"]
["","SEER","","","","","5.98","5.76"]
["","Årlig energiförbrukning","","kWh/a","","","292","347"]
["Rumsvärme (medelklimat)","Energieffektivitetsklass","","","","","A","A+"]
["","Kapacitet","Pdesign","kW","","","3.84","3.96"]
["","SCOP/A","","","","","3.90","4.04"]
["","Pdh Värmekapacitet vid -10°","","kW","","","3.51","3.66"]
["","Årlig energiförbrukning","","kWh/a","","","1377","1372"]