{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":28,"n_cols":6,"rows_kept":28,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FFA-A / RXS-L3"]
[]
[]
[]
[]
["","","","","FFA25A2VEB / RXS25L3V1B","FFA35A2VEB / RXS35L3V1B"]
["Nedkylningskapacitet","Nom.","","kW","2.50","3.40"]
["Rumskyla","SEER","","","6.11","6.32"]
["","Årlig energiförbrukning","","kWh/a","143","188"]
["","Kapacitet","Pdesign","kW","2.50","3.40"]
["","Energieffektivitetsklass","","","A++","A++"]
["Rumsvärme (medelklimat)","Kapacitet","Pdesign","kW","2.31","3.10"]
["","SCOP/A","","","4.24","4.10"]
["","Energieffektivitetsklass","","","A+","A+"]
["","Årlig energiförbrukning","","kWh/a","763","1,059"]
["Piping connections","Vätska","YD","mm","6.35","6.35"]
["","Gas","YD","mm","9.50","9.50"]
["","Kondensvatten","OD","mm","VP20 (Ytterdiameter 26, Innerdiameter 20)","VP20 (Ytterdiameter 26, Innerdiameter 20)"]
["Nominell verkningsgrad","EER köldfaktor","","","4.53","3.78"]
["","Årlig energiförbrukning","","kWh","276","450"]
["","COP","","","3.90","3.50"]
["","Energimärkningsdirektiv","Kyla","","A","A"]
["","","Värme","","A","A"]
["Värmekapacitet","Nom.","","kW","3.20","4.20"]
["Anm:","","","","(1) - Nominell kylkapacitet baseras på: inomhustemperatur: 27°CTT, 19°CVT, utomhustemperatur: 35 °CTT, ekvivalent köldmedierörledning: 5 m, nivåskillnad: 0 m.","(1) - Nominell kylkapacitet baseras på: inomhustemperatur: 27°CTT, 19°CVT, utomhustemperatur: 35 °CTT, ekvivalent köldmedierörledning: 5 m, nivåskillnad: 0 m."]
["","","","","(2) - Nominella värmekapaciteter baseras på: inomhustemperatur: 20°CTT, utomhustemperatur: 7 °CTT, 6 °CVT, ekvivalent köldmedierörledning: 5m, nivåskillnad: 0 m.","(2) - Nominella värmekapaciteter baseras på: inomhustemperatur: 20°CTT, utomhustemperatur: 7 °CTT, 6 °CVT, ekvivalent köldmedierörledning: 5m, nivåskillnad: 0 m."]
["","","","","(3) - Se separat ritning för driftsområde","(3) - Se separat ritning för driftsområde"]
["","","","","(4) - Se separata ritningar för elektriska data","(4) - Se separata ritningar för elektriska data"]