{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":29,"n_cols":7,"rows_kept":29,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FFA-A / RZASG-MV1"]
[]
[]
[]
[]
["","","","","FFA35A2VEB / FFA35A2VEB / RZASG71M2V1B","FFA35A2VEB / FFA35A2VEB / FFA35A2VEB / RZASG100M7V1B","FFA50A2VEB / FFA50A2VEB / RZASG100M7V1B"]
["Kylkapacitet","Nom.","","kW","6.80 (1)"]
["Rumskyla","SEER","","","6.12"]
["","Årlig energiförbrukning","","kWh/a","389"]
["","Kapacitet","Pdesign","kW","6.80"]
["","Energieffektivitetsklass","","","A++"]
["Rumsvärme (medelklimat)","Kapacitet","Pdesign","kW","4.50"]
["","SCOP/A","","","3.84"]
["","Energieffektivitetsklass","","","A"]
["","Årlig energiförbrukning","","kWh/a","1,641"]
["Värmekapacitet","Nom.","","kW","7.50 (2)"]
["Anm:","","","","(1) - Kyla: T2: inomhustemp. 26,6 °CTT, 19,4 °CVT, utomhustemperatur. 48°CTT [Btu/hr/W]","(1) - Nominell kylkapacitet baseras på: inomhustemp.: 27°CTT, 19°CVT, utomhustemperatur: 35 °CTT, ekvivalent köldmedierörledning: 5 m, nivåskillnad: 0 m.","(1) - Nominell kylkapacitet baseras på: inomhustemp.: 27°CTT, 19°CVT, utomhustemperatur: 35 °CTT, ekvivalent köldmedierörledning: 5 m, nivåskillnad: 0 m."]
["","","","","(2) - Nominella värmekapaciteter baseras på: inomhustemperatur: 20°CTT, utomhustemperatur: 7 °CTT, 6 °CVT, ekvivalent köldmedierörledning: 5m, nivåskillnad: 0 m.","(2) - Nominella värmekapaciteter baseras på: inomhustemperatur: 20°CTT, utomhustemperatur: 7 °CTT, 6 °CVT, ekvivalent köldmedierörledning: 5m, nivåskillnad: 0 m.","(2) - Nominella värmekapaciteter baseras på: inomhustemperatur: 20°CTT, utomhustemperatur: 7 °CTT, 6 °CVT, ekvivalent köldmedierörledning: 5m, nivåskillnad: 0 m."]
["Utomhusdel","","","","","RZASG100M7V1B","RZASG100M7V1B"]
["Kylkapacitet","Nom.","","kW","","9.50","9.50"]
["Värmekapacitet","Nom.","","kW","","10.8","10.8"]
["Rumskyla","Energieffektivitetsklass","","","","A++","A"]
["","Kapacitet","Pdesign","kW","","9.50","9.50"]
["","SEER","","","","6.24","5.49"]
["","Årlig energiförbrukning","","kWh/a","","533","606"]
["Rumsvärme (medelklimat)","Energieffektivitetsklass","","","","A","A"]
["","Kapacitet","Pdesign","kW","","6.00","6.00"]
["","SCOP/A","","","","3.82","3.90"]
["","Årlig energiförbrukning","","kWh/a","","2199","2154"]