{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":21,"n_cols":8,"rows_kept":21,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FFQ-B9V / RXS-K"]
[]
[]
[]
[]
["","","","","FFQ25B9V1B / RXS25K2V1B","FFQ25B9V1B / RXS25K3V1B","FFQ35B9V1B / RXS35K2V1B","FFQ50B9V1B / RXS50K2V1B"]
["Kylkapacitet","Nom.","","kW","2.50 (3)","2.50 (3)","3.4 (3)","4.7 (3)"]
["Röranslutningar","Vätska","YD","mm","","","6.35","6.35"]
["","Gas","YD","mm","","","9.5","12.7"]
["","Kondensvatten","YD","mm","","","VP20 (Ytterdiameter 26, Innerdiameter 20)","VP20 (Ytterdiameter 26, Innerdiameter 20)"]
["Nominell verkningsgrad","Årlig energiförbrukning","","kWh","365","365","650","900"]
["","EER köldfaktor","","","3.43","3.43","2.62","2.61"]
["","COP","","","3.48","3.48","2.81","2.81"]
["","Energimärkningsdirektiv","Kyla","","A","A","D","D"]
["","","Värme","","B","B","D","D"]
["Värmekapacitet","Nom.","","kW","3.20 (4)","3.20 (4)","4.5 (4)","5.5 (4)"]
["Anm:","","","","(1) - Energiklass: skala från A (mest effektiv) till G (mindre effektiv)","(1) - EER/COP enligt Eurovent 2012, endast för användning utanför EU","(1) - EER/COP enligt Eurovent 2012, endast för användning utanför EU","(1) - EER/COP enligt Eurovent 2012, endast för användning utanför EU"]
["","","","","(2) - Årlig energiförbrukning: baserat på en genomsnittlig användning av 500 driftstimmar per år vid full belastning (nominella förhållanden)","(2) - Nominell verkningsgrad: kyla vid 35°/27° nominell last, värme vid 7°/20° nominell last","(2) - Nominell verkningsgrad: kyla vid 35°/27° nominell last, värme vid 7°/20° nominell last","(2) - Nominell verkningsgrad: kyla vid 35°/27° nominell last, värme vid 7°/20° nominell last"]
["","","","","(3) - Kyla: inomhustemperatur. 27 °CTT, 19,0 °CVT, utomhustemperatur. 35 °CTT; ekvivalent rörledningslängd: 5 m, nivåskillnad: 0 m"]
["","","","","(4) - Värme: inomhustemperatur. 20 °CTT; utomhustemperatur 7°CTT, 6°CVT; ekvivalent köldmedierörledning: 5m, nivåskillnad: 0 m"]
["","","","","(5) - Nominell verkningsgrad: kyla vid 35°/27° nominell last, värme vid 7°/20° nominell last"]