{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":6,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHA-A(9) / RXS-L3"]
[]
[]
[]
[]
["","","","","FHA35AVEB9 / RXS35L3V1B","FHA35AVEB99 / RXS35L3V1B"]
["Kylkapacitet","Nom.","","kW","3.40","3.40"]
["Rumskyla","Årlig energiförbrukning","","kWh/a","","193"]
["","Kapacitet","Pdesign","kW","","3.40"]
["Rumsvärme (medelklimat)","Kapacitet","Pdesign","kW","","3.10"]
["","Årlig energiförbrukning","","kWh/a","","981"]
["Nominell verkningsgrad","Årlig energiförbrukning","","kWh","459","459"]
["","EER köldfaktor","","","3.70","3.70"]
["","COP","","","4.08","4.08"]
["","Energimärkningsdirektiv","Kyla","","A","A"]
["","","Värme","","A","A"]
["Värmekapacitet","Nom.","","kW","4.00","4.00"]
["Anm:","","","","(1) - \"Code du travail\" applikationer avser icke officiella byggnader (tex. kontor).","(1) - Nominell kylkapacitet baseras på: inomhustemperatur: 27°CTT, 19°CVT, utomhustemperatur: 35 °CTT, ekvivalent köldmedierörledning: 5 m, nivåskillnad: 0 m."]
["","","","","(2) - Nominella värmekapaciteter baseras på: inomhustemperatur: 20°CTT, utomhustemperatur: 7 °CTT, 6 °CVT, ekvivalent köldmedierörledning: 5m, nivåskillnad: 0 m.","(2) - Nominella värmekapaciteter baseras på: inomhustemperatur: 20°CTT, utomhustemperatur: 7 °CTT, 6 °CVT, ekvivalent köldmedierörledning: 5m, nivåskillnad: 0 m."]
["","","","","(3) - Se separat ritning för driftsområde","(3) - Se separat ritning för driftsområde"]
["","","","","(4) - Se separata ritningar för elektriska data","(4) - Se separata ritningar för elektriska data"]
["Rumskyla","SEER","","","","6.18"]
["","Energieffektivitetsklass","","","","A++"]
["Rumsvärme (medelklimat)","SCOP/A","","","","4.43"]
["","Energieffektivitetsklass","","","","A+"]