{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":42,"n_cols":7,"rows_kept":42,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHA-A / RXM-M9"]
[]
[]
[]
[]
["","","","","FHA35AVEB / RXM35M3V1B9","FHA50AVEB / RXM50M3V1B9","FHA60AVEB / RXM60M3V1B9"]
["Kylkapacitet","Nom.","","kW","3.40"]
["Rumskyla","SEER","","","6.24"]
["","Årlig energiförbrukning","","kWh/a","191"]
["","Kapacitet","Pdesign","kW","3.40"]
["","Energieffektivitetsklass","","","A++"]
["Rumsvärme (medelklimat)","Kapacitet","Pdesign","kW","3.10"]
["","SCOP/A","","","4.43"]
["","Energieffektivitetsklass","","","A+"]
["","Årlig energiförbrukning","","kWh/a","979"]
["Nominell verkningsgrad","Årlig energiförbrukning","","kWh","456"]
["","EER köldfaktor","","","3.73"]
["","COP","","","4.08"]
["","Energimärkningsdirektiv","Kyla","","A"]
["","","Värme","","A"]
["Värmekapacitet","Nom.","","kW","4.00"]
["Anm:","","","","(1) - Se separata ritningar för elektriska data"]
["","","","","(2) - Se separat ritning för driftsområde"]
["","","","","(3) - Nominell kylkapacitet baseras på: inomhustemp.: 27°CTT, 19°CVT, utomhustemperatur: 35 °CTT, ekvivalent köldmedierörledning: 5 m, nivåskillnad: 0 m."]
["","","","","(4) - Nominella värmekapaciteter baseras på: inomhustemperatur: 20°CTT, utomhustemperatur: 7 °CTT, 6 °CVT, ekvivalent köldmedierörledning: 5m, nivåskillnad: 0 m."]
["Utomhusdel","","","","","RXM50M3V1B9","RXM60M3V1B9"]
["Kylkapacitet","Nom.","","kW","","5.00","5.70"]
["Värmekapacitet","Nom.","","kW","","6.00","7.20"]
["Nominell verkningsgrad","EER köldfaktor","","","","3.21","3.29"]
["","COP","","","","3.35","3.32"]
["","Årlig energiförbrukning","","kWh","","780","867"]
["","Energimärkningsdirektiv","Kyla","","","B","A"]
["","","Värme","","","C","C"]
["Rumskyla","Energieffektivitetsklass","","","","A+","A+"]
["","Kapacitet","Pdesign","kW","","5.00","5.70"]
["","SEER","","","","5.92","6.08"]
["","Årlig energiförbrukning","","kWh/a","","295","328"]
["Rumsvärme (medelklimat)","Energieffektivitetsklass","","","","A","A"]
["","Kapacitet","Pdesign","kW","","4.35","4.71"]
["","SCOP/A","","","","3.86","3.87"]
["","Pdh Värmekapacitet vid -10°","","kW","","3.85","4.08"]
["","Årlig energiförbrukning","","kWh/a","","1578","1704"]