{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":6,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHA-A / RXM-N"]
[]
[]
[]
[]
["","","","","FHA50AVEB / RXM50N2V1B","FHA60AVEB / RXM60N2V1B"]
["Nedkylningskapacitet","Nom.","","kW","5.00","5.70"]
["Rumskyla","Årlig energiförbrukning","","kWh/a","","328"]
["","Kapacitet","Pdesign","kW","","5.70"]
["Rumsvärme (medelklimat)","Kapacitet","Pdesign","kW","","4.71"]
["","Årlig energiförbrukning","","kWh/a","","1,704"]
["Nominell verkningsgrad","Årlig energiförbrukning","","kWh","780","867"]
["","EER köldfaktor","","","3.21","3.29"]
["","COP","","","3.35","3.32"]
["","Energimärkningsdirektiv","Kyla","","A","A"]
["","","Värme","","C","C"]
["Värmekapacitet","Nom.","","kW","6.00","7.20"]
["Anm:","","","","(1) - Se separat ritning för driftsområde","(1) - Se separat ritning för driftsområde"]
["","","","","(2) - Se separata ritningar för elektriska data","(2) - Se separata ritningar för elektriska data"]
["","","","","(3) - Nominell kylkapacitet baseras på: inomhustemperatur: 27°CTT, 19°CVT, utomhustemperatur: 35 °CTT, ekvivalent köldmedierörledning: 5 m, nivåskillnad: 0 m.","(3) - Nominell kylkapacitet baseras på: inomhustemp.: 27°CTT, 19°CVT, utomhustemperatur: 35 °CTT, ekvivalent köldmedierörledning: 5 m, nivåskillnad: 0 m."]
["","","","","(4) - Nominella värmekapaciteter baseras på: inomhustemperatur: 20°CTT, utomhustemperatur: 7 °CTT, 6 °CVT, ekvivalent köldmedierörledning: 5m, nivåskillnad: 0 m.","(4) - Nominella värmekapaciteter baseras på: inomhustemperatur: 20°CTT, utomhustemperatur: 7 °CTT, 6 °CVT, ekvivalent köldmedierörledning: 5m, nivåskillnad: 0 m."]
["Rumskyla","Energieffektivitetsklass","","","","A+"]
["","SEER","","","","6.08"]
["Rumsvärme (medelklimat)","Energieffektivitetsklass","","","","A"]
["","SCOP/A","","","","3.87"]