{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":18,"n_cols":11,"rows_kept":18,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHA-A / RZQSG-L3/9V1"]
[]
[]
[]
[]
["","","","","FHA71AVEB / RZQSG71L3V1B","FHA50AVEB / FHA50AVEB / FHA50AVEB / RZQSG125L9V1B","FHA50AVEB / FHA50AVEB / RZQSG100L9V1B","FHA60AVEB / FHA60AVEB / RZQSG125L9V1B","FHA35AVEB / FHA35AVEB / RZQSG71L3V1B","FHA35AVEB / FHA35AVEB / FHA35AVEB / RZQSG100L9V1B","FHA35AVEB / FHA35AVEB / FHA35AVEB / FHA35AVEB / RZQSG125L9V1B"]
["Rumskyla","Årlig energiförbrukning","","kWh/a","","","","","467","652","875"]
["","Kapacitet","Pdesign","kW","","","","","6.80","9.50","12.0"]
["Rumsvärme (medelklimat)","Kapacitet","Pdesign","kW","","","","","6.00","7.60","7.60"]
["","Årlig energiförbrukning","","kWh/a","","","","","2,211","2,800","2,800"]
["Intervall för energieffektivitet","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D"]
["Rumskyla","SEER","","","","","","","5.10","5.10","4.80"]
["","Energieffektivitetsklass","","","","","","","A","A","B"]
["Rumsvärme (medelklimat)","SCOP/A","","","","","","","3.80","3.80","3.80"]
["","Energieffektivitetsklass","","","","","","","A","A","A"]
["Anm:","","","","","","","","(1) - Kyla: inomhustemperatur. 27 °CTT, 19 °CVT; utomhustemperatur 35 °CTT; ekvivalent rörledningslängd: 7,5 m, nivåskillnad: 0 m","(1) - Kyla: inomhustemperatur. 27 °CTT, 19 °CVT; utomhustemperatur 35 °CTT; ekvivalent rörledningslängd: 7,5 m, nivåskillnad: 0 m","(1) - Kyla: inomhustemperatur. 27 °CTT, 19 °CVT; utomhustemperatur 35 °CTT; ekvivalent rörledningslängd: 7,5 m, nivåskillnad: 0 m"]
["","","","","","","","","(2) - Värme: inomhustemperatur. 20 °CTT; utomhustemperatur 7°CTT, 6°CVT; ekvivalent köldmedierörledning: 7,5 m, nivåskillnad: 0 m","(2) - Värme: inomhustemperatur. 20 °CTT; utomhustemperatur 7°CTT, 6°CVT; ekvivalent köldmedierörledning: 7,5 m, nivåskillnad: 0 m","(2) - Värme: inomhustemperatur. 20 °CTT; utomhustemperatur 7°CTT, 6°CVT; ekvivalent köldmedierörledning: 7,5 m, nivåskillnad: 0 m"]
["","","","","","","","","(3) - EER/COP enligt Eurovent 2012, endast för användning utanför EU","(3) - EER/COP enligt Eurovent 2012, endast för användning utanför EU","(3) - EER/COP enligt Eurovent 2012, endast för användning utanför EU"]