{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":13,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHQ-C / RZQSG-L3/9V1"]
[]
[]
[]
[]
["","","","","FHQ71CAVEB / RZQSG71L3V1B","FHQ100CAVEB / RZQSG100L9V1B","FHQ35CAVEB / FHQ35CAVEB / FHQ35CAVEB / RZQSG100L9V1B","FHQ50CAVEB / FHQ50CAVEB / RZQSG100L9V1B","FHQ125CAVEB / RZQSG125L9V1B","FHQ35CAVEB / FHQ35CAVEB / FHQ35CAVEB / FHQ35CAVEB / RZQSG125L9V1B","FHQ50CAVEB / FHQ50CAVEB / FHQ50CAVEB / RZQSG125L9V1B","FHQ60CAVEB / FHQ60CAVEB / RZQSG125L9V1B","FHQ140CAVEB / RZQSG140L9V1B"]
["Kylkapacitet","Nom.","","kW","6.8","9.5","","","12.0","","","","13.4"]
["Rumskyla","SEER","","","5.61","5.61","5.10","5.10","5.61","4.80","4.80","4.80"]
["","Årlig energiförbrukning","","kWh/a","424","593","652","652","749","875","875","875"]
["","Kapacitet","Pdesign","kW","6.80","9.50","9.50","9.50","12.00","12.00","12.00","12.00"]
["","Energieffektivitetsklass","","","A+","A+","B","B","A+","B","B","B"]
["Rumsvärme (medelklimat)","Kapacitet","Pdesign","kW","7.60","7.60","7.60","7.60","7.60","7.60","7.60","7.60"]
["","SCOP/A","","","3.90","3.91","3.80","3.80","4.01","3.80","3.80","3.80"]
["","Energieffektivitetsklass","","","A","A","A","A","A+","A","A","A"]
["","Årlig energiförbrukning","","kWh/a","2,727","2,722","2,800","2,800","2,654","2,800","2,800","2,800"]
["Nominell verkningsgrad","Årlig energiförbrukning","","kWh","985","1,480","","","2,075"]
["","EER köldfaktor","","","3.46","3.21","","","2.89","","","","3.01"]
["","COP","","","4.00","3.61","","","3.62","","","","3.41"]
["","Energimärkningsdirektiv","Kyla","","A","A","","","C"]
["","","Värme","","A","A","","","A"]
["Värmekapacitet","Nom.","","kW","7.5","10.8","","","13.5","","","","15.5"]
["Anm:","","","","(1) - EER/COP enligt Eurovent 2012, endast för användning utanför EU","(1) - EER/COP enligt Eurovent 2012, endast för användning utanför EU","","","(1) - EER/COP enligt Eurovent 2012, endast för användning utanför EU","","","","(1) - EER/COP enligt Eurovent 2012, endast för användning utanför EU"]
["","","","","(2) - Nominell verkningsgrad: kyla vid 35°/27° nominell last, värme vid 7°/20° nominell last","(2) - Nominell verkningsgrad: kyla vid 35°/27° nominell last, värme vid 7°/20° nominell last","","","(2) - Nominell verkningsgrad: kyla vid 35°/27° nominell last, värme vid 7°/20° nominell last","","","","(2) - Nominell verkningsgrad: kyla vid 35°/27° nominell last, värme vid 7°/20° nominell last"]
["","","","","","","(1) - EER/COP enligt Eurovent 2012, endast för användning utanför EU","(1) - EER/COP enligt Eurovent 2012, endast för användning utanför EU","","(1) - EER/COP enligt Eurovent 2012, endast för användning utanför EU","(1) - EER/COP enligt Eurovent 2012, endast för användning utanför EU","(1) - EER/COP enligt Eurovent 2012, endast för användning utanför EU"]