{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":38,"n_cols":9,"rows_kept":38,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FNA-A9"]
[]
[]
[]
[]
["","","","","","FNA25A2VEB9","FNA35A2VEB9","FNA50A2VEB9","FNA60A2VEB9"]
["Ljudtrycksnivå","Värme","","Hög","dBA","33.0","33.0","36.0","36.0"]
["","","","Nom.","dBA","31.0","31.0","33.0","33.0"]
["","","","Låg","dBA","28.0","28.0","30.0","30.0"]
["","Kyla","","Medel","dBA","31.0","31.0","33.0","33.0"]
["","","","Låg","dBA","28.0","28.0","30.0","30.0"]
["","","","Hög","dBA","33.0","33.0","36.0","36.0"]
["Styrsystem","Wired remote control","","","","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52"]
["","Infrared remote control","","","","BRC4C65","BRC4C65","BRC4C65","BRC4C65"]
["Röranslutningar","Vätska","","YD","mm","6.35","6.35","6.35","6.35"]
["","Gas","","YD","mm","9.52","9.52","12.7","12.7"]
["","Kondensvatten","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Ljudeffektsnivå","Kyla","","","dBA","53.0","53.0","56.0","56.0"]
["Mått","Enhet","","Bredd","mm","790","790","1,190","1,190"]
["","","","Djup","mm","200","200","200","200"]
["","","","Höjd","mm","620, 720 (1)","620, 720 (1)","620, 720 (1)","620, 720 (1)"]
["Hölje","Material","","","","Galvaniserad stålplåt","Galvaniserad stålplåt","Galvaniserad stålplåt","Galvaniserad stålplåt"]
["","Färg","","","","Omålat","Omålat","Omålat","Omålat"]
["Vikt","Enhet","","","kg","23.0","23.0","30.0","30.0"]
["Fläkt","Yttre statiskt tryck","","Hög","Pa","48","48","49","49"]
["","","","Nom.","Pa","30","30","40","40"]
["","Luftflödeshastighet","Värme","Hög","m³/min","8.7","8.7","16.0","16.0"]
["","","","Låg","m³/min","7.3","7.3","13.5","13.5"]
["","","","Nom.","m³/min","8.0","8.0","14.8","14.8"]
["","","Kyla","Låg","m³/min","7.3","7.3","13.5","13.5"]
["","","","Nom.","m³/min","8.0","8.0","14.8","14.8"]
["","","","Hög","m³/min","8.7","8.7","16.0","16.0"]
["Power supply","Fas","","","","1~","1~","1~","1~"]
["","Namn","","","","VE","VE","VE","VE"]
["","Frequency","","","Hz","50/60","50/60","50/60","50/60"]
["","Spänning","","","V","220-240/220","220-240/220","220-240/220","220-240/220"]
["Anm:","","","","","(1) - Inklusive installationsben","(1) - Inklusive installationsben","(1) - Inklusive installationsben","(1) - Inklusive installationsben"]
["","","","","","(2) - Ljudeffektsnivån är ett absolut värde som anger vilken effekt en ljudkälla genererar.","(2) - Ljudeffektsnivån är ett absolut värde som anger vilken effekt en ljudkälla genererar.","(2) - Ljudeffektsnivån är ett absolut värde som anger vilken effekt en ljudkälla genererar.","(2) - Ljudeffektsnivån är ett absolut värde som anger vilken effekt en ljudkälla genererar."]