{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":34,"n_cols":8,"rows_kept":34,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FNQ-A"]
[]
[]
[]
[]
["","","","","FNQ25A2VEB","FNQ35A2VEB","FNQ50A2VEB","FNQ60A2VEB"]
["Ljudtrycksnivå","Värme","Hög","dBA","33","33","36","36"]
["","","Nom.","dBA","31","31","33","33"]
["","","Låg","dBA","28","28","30","30"]
["","Kyla","Låg","dBA","28","28","30","30"]
["","","Hög","dBA","33","33","36","36"]
["","","Nom.","dBA","31","31","33","33"]
["Köldmedium","GWP","","","2,087.5","2,087.5","2,087.5","2,087.5"]
["Styrsystem","Kabelansluten fjärrkontroll","","","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B"]
["","Infrared remote control","","","BRC4C65","BRC4C65","BRC4C65","BRC4C65"]
["Kylkapacitet","Total kapacitet","Nom.","kW","2.6","3.4","5.0","6.0"]
["Röranslutningar","Vätska","YD","mm","6.35","6.35","6.35","6.35"]
["","Gas","YD","mm","9.52","9.52","12.7","12.7"]
["","Kondensvatten","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Ljudeffektsnivå","Kyla","","dBA","53","53","56","56"]
["Mått","Enhet","Bredd","mm","790","790","1,190","1,190"]
["","","Djup","mm","200","200","200","200"]
["","","Höjd","mm","620, 720 (2)","620, 720 (2)","620, 720 (2)","620, 720 (2)"]
["Hölje","Material","","","Galvaniserad stålplåt","Galvaniserad stålplåt","Galvaniserad stålplåt","Galvaniserad stålplåt"]
["","Färg","","","Omålat","Omålat","Omålat","Omålat"]
["Vikt","Enhet","","kg","23","23","30","30"]
["Fläkt","Yttre statiskt tryck","Hög","Pa","48","48","49","49"]
["","","Nom.","Pa","30","30","40","40"]
["Värmekapacitet","Total capacity","Nom.","kW","3.2","4.0","5.8","7.0"]
["Power supply","Fas","","","1~","1~","1~","1~"]
["","Frequency","","Hz","50/60","50/60","50/60","50/60"]
["","Spänning","","V","220-240/220","220-240/220","220-240/220","220-240/220"]
["Anm:","","","","(1) - Ljudeffektsnivån är ett absolut värde som anger vilken effekt en ljudkälla genererar.","(1) - Ljudeffektsnivån är ett absolut värde som anger vilken effekt en ljudkälla genererar.","(1) - Ljudeffektsnivån är ett absolut värde som anger vilken effekt en ljudkälla genererar.","(1) - Ljudeffektsnivån är ett absolut värde som anger vilken effekt en ljudkälla genererar."]
["","","","","(2) - Inklusive installationsben","(2) - Inklusive installationsben","(2) - Inklusive installationsben","(2) - Inklusive installationsben"]