{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":40,"n_cols":7,"rows_kept":40,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXA-CW / RXA-A8"]
[]
[]
[]
[]
["","","","","FTXA20C2V1BW / RXA20A5V1B8","FTXA25C2V1BW / RXA25A5V1B8","FTXA35C2V1BW / RXA35A5V1B8"]
["Kylkapacitet","Min.","","kW","","1.30","1.40"]
["","Nom.","","kW","","2.50","3.40"]
["","Max.","","kW","","3.20","4.00"]
["Uppvärmningseffekt","Min.","","kW","","1.30","1.40"]
["","Nom.","","kW","","2.80","4.00"]
["","Max.","","kW","","4.70","5.20"]
["Nominell verkningsgrad","Årlig energiförbrukning","","kWh","","280","389"]
["","COP","","","","5.00","4.04"]
["","EER köldfaktor","","","","4.46","4.37"]
["","Energimärkningsdirektiv","Kyla","","","A","A"]
["","","Värme","","","A","A"]
["Anm:","","","","","(1) - Nominell kylkapacitet baseras på: inomhustemperatur: 27°CTT, 19°CVT, utomhustemperatur: 35 °CTT, ekvivalent köldmedierörledning: 5 m, nivåskillnad: 0 m.","(1) - Nominell kylkapacitet baseras på: inomhustemperatur: 27°CTT, 19°CVT, utomhustemperatur: 35 °CTT, ekvivalent köldmedierörledning: 5 m, nivåskillnad: 0 m."]
["","","","","","(2) - Nominella värmekapaciteter baseras på: inomhustemperatur: 20°CTT, utomhustemperatur: 7 °CTT, 6 °CVT, ekvivalent köldmedierörledning: 5m, nivåskillnad: 0 m.","(2) - Nominella värmekapaciteter baseras på: inomhustemperatur: 20°CTT, utomhustemperatur: 7 °CTT, 6 °CVT, ekvivalent köldmedierörledning: 5m, nivåskillnad: 0 m."]
["","","","","","(3) - Se separat ritning för driftsområde","(3) - Se separat ritning för driftsområde"]
["Kylkapacitet","Min.","","kW","1.30"]
["","Nom.","","kW","2.00"]
["","Max.","","kW","2.60"]
["Värmekapacitet","Min.","","kW","1.30"]
["","Nom.","","kW","2.50"]
["","Max.","","kW","3.50"]
["Nominell verkningsgrad","EER köldfaktor","","","4.70"]
["","COP","","","5.00"]
["","Årlig energiförbrukning","","kWh","213"]
["","Energimärkningsdirektiv","Kyla","","A"]
["","","Värme","","A"]
["Rumskyla","Energieffektivitetsklass","","","A+++"]
["","Kapacitet","Pdesign","kW","2.00"]
["","SEER","","","8.75"]
["","Årlig energiförbrukning","","kWh/a","80"]
["Rumsvärme (medelklimat)","Energieffektivitetsklass","","","A+++"]
["","Kapacitet","Pdesign","kW","2.40"]
["","SCOP/A","","","5.15"]
["","Pdh Värmekapacitet vid -10°","","kW","2.04"]
["","Årlig energiförbrukning","","kWh/a","652"]