{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":17,"n_cols":6,"rows_kept":17,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXF-A / 3MXF-A"]
[]
[]
[]
[]
["","","","","FTXF20A5V1B / FTXF20A5V1B / FTXF20A5V1B / 3MXF52A2V1B","FTXF20A5V1B / FTXF25A5V1B / FTXF25A5V1B / 3MXF68A2V1B"]
["Kylkapacitet","Min.","","kW","1.80","2.00"]
["","Max.","","kW","7.00","7.20"]
["","Nom.","","kW","5.20","6.80"]
["Nominell verkningsgrad","Årlig energiförbrukning","","kWh","634","977"]
["","EER köldfaktor","","","4.10","3.48"]
["","COP","","","3.93","3.82"]
["","Energimärkningsdirektiv","Kyla","","A","A"]
["","","Värme","","A","A"]
["Värmekapacitet","Nom.","","kW","6.80","8.60"]
["","Min.","","kW","1.30","2.20"]
["","Max.","","kW","8.00","10.50"]