{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":19,"n_cols":6,"rows_kept":19,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXF-B / RXF-B"]
[]
[]
[]
[]
["","","","","FTXF20B5V1B / RXF20B5V1B","FTXF25B5V1B / RXF25B5V1B"]
["Kylkapacitet","Min.","","kW","1.3","1.3"]
["","Max.","","kW","2.6","3.0"]
["","Nom.","","kW","2.00","2.50"]
["Nominell verkningsgrad","EER köldfaktor","","","3.94","3.30"]
["","COP","","","4.19","4.01"]
["","Energimärkningsdirektiv","Kyla","","A","A"]
["","","Värme","","A","A"]
["Uppvärmningseffekt","Nom.","","kW","2.50","2.80"]
["","Min.","","kW","1.30","1.30"]
["","Max.","","kW","3.50","4.00"]
["Anm:","","","","(1) - Nominell kylkapacitet baseras på: inomhustemperatur: 27°CTT, 19°CVT, utomhustemperatur: 35 °CTT, ekvivalent köldmedierörledning: 5 m, nivåskillnad: 0 m.","(1) - Nominell kylkapacitet baseras på: inomhustemperatur: 27°CTT, 19°CVT, utomhustemperatur: 35 °CTT, ekvivalent köldmedierörledning: 5 m, nivåskillnad: 0 m."]
["","","","","(2) - Nominella värmekapaciteter baseras på: inomhustemperatur: 20°CTT, utomhustemperatur: 7 °CTT, 6 °CVT, ekvivalent köldmedierörledning: 5m, nivåskillnad: 0 m.","(2) - Nominella värmekapaciteter baseras på: inomhustemperatur: 20°CTT, utomhustemperatur: 7 °CTT, 6 °CVT, ekvivalent köldmedierörledning: 5m, nivåskillnad: 0 m."]
["","","","","(3) - Se separata ritningar för elektriska data","(3) - Se separata ritningar för elektriska data"]