{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":12,"n_cols":6,"rows_kept":12,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXG-LW / RXS-L1"]
[]
[]
[]
[]
["","","","FTXG25LV1BW / RXS25L3V1B1","FTXG35LV1BW / RXS35L3V1B1","FTXG50LV1BW / RXS50L2V1B1"]
["Kylkapacitet","Nom.","kW","2.50 (1)","3.40 (1)","4.50 (1)"]
["Nominell verkningsgrad","EER köldfaktor","","4.30","3.87","3.58"]
["","COP","","4.10","3.72","3.58"]
["Värmekapacitet","Nom.","kW","3.20 (2)","4.00 (2)","4.85 (2)"]
["Anm:","","","(1) - Inomhustemperatur: 27°CTT, 19°CVT; utomhustemperatur : 35°CTT, 24°CVT","(1) - Inomhustemperatur: 27°CTT, 19°CVT; utomhustemperatur : 35°CTT, 24°CVT","(1) - Inomhustemperatur: 27°CTT, 19°CVT; utomhustemperatur : 35°CTT, 24°CVT"]
["","","","(2) - Inomhustemperatur: 20°CTT, 15°CVT; utomhustemperatur : 7°CTT, 6°CVT.","(2) - Inomhustemperatur: 20°CTT, 15°CVT; utomhustemperatur : 7°CTT, 6°CVT.","(2) - Inomhustemperatur: 20°CTT, 15°CVT; utomhustemperatur : 7°CTT, 6°CVT."]