{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":35,"n_cols":8,"rows_kept":35,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXJ-AB / RXJ-M9"]
[]
[]
[]
[]
["","","","","FTXJ20A2V1BB / RXJ20M5V1B9","FTXJ25A2V1BB / RXJ25M5V1B9","FTXJ35A2V1BB  / RXJ35M5V1B9","FTXJ35A2V1BB / RXJ35M5V1B9"]
["Nedkylningskapacitet","Nom.","","kW","","","3.50"]
["Nominell verkningsgrad","Årlig energiförbrukning","","kWh","","","428"]
["","EER köldfaktor","","","","","4.09"]
["","COP","","","","","4.04"]
["","Energimärkningsdirektiv","Kyla","","","","A"]
["","","Värme","","","","A"]
["Värmekapacitet","Nom.","","kW","","","4.00"]
["Anm:","","","","","","(1) - Se separat ritning för driftsområde"]
["","","","","","","(2) - Se separata ritningar för elektriska data"]
["","","","","","","(3) - Nominell kylkapacitet baseras på: inomhustemperatur: 27°CTT, 19°CVT, utomhustemperatur: 35 °CTT, ekvivalent köldmedierörledning: 5 m, nivåskillnad: 0 m."]
["","","","","","","(4) - Nominella värmekapaciteter baseras på: inomhustemperatur: 20°CTT, utomhustemperatur: 7 °CTT, 6 °CVT, ekvivalent köldmedierörledning: 5m, nivåskillnad: 0 m."]
["Outdoor unit","","","","RXJ20M5V1B9","RXJ25M5V1B9","","RXJ35M5V1B9"]
["Kylkapacitet","Nom.","","kW","2.30","2.40","","3.50"]
["Värmekapacitet","Nom.","","kW","2.50","3.20","","4.00"]
["Nominell verkningsgrad","EER köldfaktor","","","4.64","4.73","","4.09"]
["","COP","","","5.00","4.57","","4.04"]
["","Årlig energiförbrukning","","kWh","248","254","","428"]
["","Energimärkningsdirektiv","Kyla","","A","A","","A"]
["","","Värme","","A","A","","A"]
["Rumskyla","Energieffektivitetsklass","","","A+++","A+++","","A++"]
["","Kapacitet","Pdesign","kW","2.30","2.40","","3.50"]
["","SEER","","","8.73","8.64","","7.19"]
["","Årlig energiförbrukning","","kWh/a","92","97","","170"]
["Rumsvärme (medelklimat)","Energieffektivitetsklass","","","A++","A++","","A++"]
["","Kapacitet","Pdesign","kW","2.10","2.70","","3.00"]
["","SCOP/A","","","4.61","4.60","","4.60"]
["","Pdh Värmekapacitet vid -10°","","kW","1.80","2.18","","2.61"]
["","Årlig energiförbrukning","","kWh/a","638","822","","913"]
["Energy Efficiency Range","","","","A+++ ~ D","A+++ ~ D","","A+++ ~ D"]