{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":5,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXJ-MW / 4MXM-N"]
[]
[]
[]
[]
["","","","","FTXJ20MV1BW / FTXJ20MV1BW / FTXJ20MV1BW / FTXJ20MV1BW / 4MXM80N2V1B"]
["Kylkapacitet","Nom.","","kW","7.50"]
["Rumskyla","SEER","","","6.92"]
["","Årlig energiförbrukning","","kWh/a","380"]
["","Kapacitet","Pdesign","kW","7.50"]
["","Energieffektivitetsklass","","","A++"]
["Rumsvärme (medelklimat)","Kapacitet","Pdesign","kW","6.46"]
["","SCOP/A","","","4.02"]
["","Energieffektivitetsklass","","","A+"]
["","Årlig energiförbrukning","","kWh/a","2,245"]
["Nominell verkningsgrad","Årlig energiförbrukning","","kWh","908"]
["","EER köldfaktor","","","4.13"]
["","COP","","","3.32"]
["","Energimärkningsdirektiv","Kyla","","A"]
["","","Värme","","C"]
["Värmekapacitet","Nom.","","kW","10.00"]
["Anm:","","","","(1) - Nominell kylkapacitet baseras på: inomhustemp.: 27°CTT, 19°CVT, utomhustemperatur: 35 °CTT, ekvivalent köldmedierörledning: 5 m, nivåskillnad: 0 m."]
["","","","","(2) - Nominella värmekapaciteter baseras på: inomhustemperatur: 20°CTT, utomhustemperatur: 7 °CTT, 6 °CVT, ekvivalent köldmedierörledning: 5m, nivåskillnad: 0 m."]
["","","","","(3) - Se separat ritning för driftsområde"]
["","","","","(4) - Se separata ritningar för elektriska data"]