{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":43,"n_cols":6,"rows_kept":43,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXLS-K3"]
[]
[]
[]
[]
["","","","","FTXLS25K3V1B","FTXLS35K3V1B"]
["Ljudtrycksnivå","Värme","Hög","dBA","47","47"]
["","","Tyst drift","dBA","19","19"]
["","","Låg","dBA","23","23"]
["","Kyla","Tyst drift","dBA","21","21"]
["","","Låg","dBA","33","33"]
["","","Hög","dBA","45","45"]
["","","Nom.","dBA","37","36"]
["","Kyla","Nom.","dBA","39","39"]
["Standardtillbehör","Installationsanvisning","","","1","1"]
["","Bruksanvisning","","","1","1"]
["","Infraröd fjärrkontroll","","","1","1"]
["","Batterier","","","2","2"]
["","Hållare för fjärrkontroll","","","1","1"]
["","Monteringsplåt","","","1","1"]
["","Fotokatalytiskt luftreningsfilter med titanapatit","","","2","2"]
["","Fästskruvar för inomhusenhet","","","2","2"]
["Styrsystem","Infrared remote control","","","ARC466A9","ARC466A9"]
["Röranslutningar","Vätska","YD","mm","6.35","6.35"]
["","Gas","YD","mm","9.5","9.5"]
["","Drain","","","18","18"]
["Ineffekt","Kyla","Nom.","kW","0.024 (2), 0.024 (3), 0.024 (4)","0.024 (2), 0.024 (3), 0.024 (4)"]
["","Värme","Nom.","kW","0.030 (2), 0.030 (3), 0.030 (4)","0.030 (2), 0.030 (3), 0.030 (4)"]
["Sound power level","Kyla","","dBA","59","59"]
["","Värme","","dBA","62","62"]
["Mått","Enhet","Bredd","mm","900","900"]
["","","Djup","mm","215","215"]
["","","Höjd","mm","298","298"]
["Hölje","Färg","","","Vit","Vit"]
["Vikt","Enhet","","kg","12","12"]
["Power supply","Fas","","","1~","1~"]
["","Frequency","","Hz","50","50"]
["","Namn","","","V1","V1"]
["","Spänning","","V","220-240","220-240"]
["Anm:","","","","(1) - Vid anslutning till en utomhusdel med multisystem, se specifikationerna för multiutomhusdelen som ska anslutas.","(1) - Vid anslutning till en utomhusdel med multisystem, se specifikationerna för multiutomhusdelen som ska anslutas."]
["","","","","(2) - 220V","(2) - 220V"]
["","","","","(3) - 230V","(3) - 230V"]
["","","","","(4) - 240V","(4) - 240V"]