{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":21,"n_cols":5,"rows_kept":21,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXM-R / RXM-N"]
[]
[]
[]
[]
["","","","","FTXM71R2V1B / RXM71N2V1B"]
["Nedkylningskapacitet","Min.","","kW","2.30"]
["","Max.","","kW","8.50"]
["","Nom.","","kW","7.10"]
["Nominell verkningsgrad","Årlig energiförbrukning","","kWh","1,172"]
["","EER köldfaktor","","","3.03"]
["","COP","","","3.19"]
["","Energimärkningsdirektiv","Kyla","","B"]
["","","Värme","","D"]
["Värmekapacitet","Nom.","","kW","8.20"]
["","Min.","","kW","2.30"]
["","Max.","","kW","10.20"]
["Anm:","","","","(1) - Se separat ritning för driftsområde"]
["","","","","(2) - Se separata ritningar för elektriska data"]
["","","","","(3) - Nominell kylkapacitet baseras på: inomhustemp.: 27°CTT, 19°CVT, utomhustemperatur: 35 °CTT, ekvivalent köldmedierörledning: 5 m, nivåskillnad: 0 m."]
["","","","","(4) - Nominella värmekapaciteter baseras på: inomhustemperatur: 20°CTT, utomhustemperatur: 7 °CTT, 6 °CVT, ekvivalent köldmedierörledning: 5m, nivåskillnad: 0 m."]