{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":40,"n_cols":7,"rows_kept":40,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXP-M / RXP-N"]
[]
[]
[]
[]
["","","","","FTXP50M2V1B / RXP50N5V1B","FTXP60M2V1B / RXP60N5V1B","FTXP71M2V1B / RXP71N5V1B"]
["Kylkapacitet","Min.","","kW","1.7","1.7"]
["","Nom.","","kW","5.0","6.0"]
["","Max.","","kW","6.0","7.0"]
["Uppvärmningseffekt","Min.","","kW","1.7","1.7"]
["","Nom.","","kW","6.0","7.0"]
["","Max.","","kW","7.7","8.0"]
["Nominell verkningsgrad","Årlig energiförbrukning","","kWh","693","912"]
["","COP","","","3.80","3.63"]
["","EER köldfaktor","","","3.61","3.29"]
["","Energimärkningsdirektiv","Kyla","","A","A"]
["","","Värme","","A","A"]
["Anm:","","","","(1) - Nominell kylkapacitet baseras på: inomhustemperatur: 27°CTT, 19°CVT, utomhustemperatur: 35 °CTT, ekvivalent köldmedierörledning: 5 m, nivåskillnad: 0 m.","(1) - Nominell kylkapacitet baseras på: inomhustemperatur: 27°CTT, 19°CVT, utomhustemperatur: 35 °CTT, ekvivalent köldmedierörledning: 5 m, nivåskillnad: 0 m.","(1) - Nominell kylkapacitet baseras på: inomhustemp.: 27°CTT, 19°CVT, utomhustemperatur: 35 °CTT, ekvivalent köldmedierörledning: 5 m, nivåskillnad: 0 m."]
["","","","","(2) - Nominella värmekapaciteter baseras på: inomhustemperatur: 20°CTT, utomhustemperatur: 7 °CTT, 6 °CVT, ekvivalent köldmedierörledning: 5m, nivåskillnad: 0 m.","(2) - Nominella värmekapaciteter baseras på: inomhustemperatur: 20°CTT, utomhustemperatur: 7 °CTT, 6 °CVT, ekvivalent köldmedierörledning: 5m, nivåskillnad: 0 m.","(2) - Nominella värmekapaciteter baseras på: inomhustemperatur: 20°CTT, utomhustemperatur: 7 °CTT, 6 °CVT, ekvivalent köldmedierörledning: 5m, nivåskillnad: 0 m."]
["Kylkapacitet","Min.","","kW","","","2.3"]
["","Nom.","","kW","","","7.1"]
["","Max.","","kW","","","7.3"]
["Värmekapacitet","Min.","","kW","","","2.3"]
["","Nom.","","kW","","","8.2"]
["","Max.","","kW","","","9.0"]
["Nominell verkningsgrad","EER köldfaktor","","","","","2.64"]
["","COP","","","","","3.19"]
["","Årlig energiförbrukning","","kWh","","","1345"]
["","Energimärkningsdirektiv","Kyla","","","","D"]
["","","Värme","","","","D"]
["Rumskyla","Energieffektivitetsklass","","","","","A++"]
["","Kapacitet","Pdesign","kW","","","7.1"]
["","SEER","","","","","6.20"]
["","Årlig energiförbrukning","","kWh/a","","","401"]
["Rumsvärme (medelklimat)","Energieffektivitetsklass","","","","","A+"]
["","Kapacitet","Pdesign","kW","","","6.20"]
["","SCOP/A","","","","","4.01"]
["","Pdh Värmekapacitet vid -10°","","kW","","","4.24"]
["","Årlig energiförbrukning","","kWh/a","","","2166"]
["Intervall för energieffektivitet","","","","","","A+++ ~ D"]