{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":34,"n_cols":6,"rows_kept":34,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXP-M9 / 2MXM-A9"]
[]
[]
[]
[]
["","","","","FTXP20M5V1B9 / FTXP20M5V1B9 / 2MXM40A2V1B9","FTXP20M5V1B9 / FTXP20M5V1B9 / 2MXM50A2V1B9"]
["Kylkapacitet","Nom.","","kW","4.00"]
["Värmekapacitet","Nom.","","kW","4.20"]
["Nominell verkningsgrad","EER köldfaktor","","","3.71"]
["","COP","","","3.75"]
["","Årlig energiförbrukning","","kWh","539"]
["","Energimärkningsdirektiv","Kyla","","A"]
["","","Värme","","A"]
["Rumskyla","Energieffektivitetsklass","","","A++"]
["","Kapacitet","Pdesign","kW","4.00"]
["","SEER","","","7.74"]
["","Årlig energiförbrukning","","kWh/a","181"]
["Rumsvärme (medelklimat)","Energieffektivitetsklass","","","A+"]
["","Kapacitet","Pdesign","kW","3.20"]
["","SCOP/A","","","4.30"]
["","Pdh Värmekapacitet vid -10°","","kW","2.46"]
["","Årlig energiförbrukning","","kWh/a","1041"]
["Intervall för energieffektivitet","","","","A+++ ~ D"]
["Anm:","","","","(1) - Nominell kylkapacitet baseras på: inomhustemp.: 27°CTT, 19°CVT, utomhustemperatur: 35 °CTT, ekvivalent köldmedierörledning: 5 m, nivåskillnad: 0 m.","(1) - Nominell kylkapacitet baseras på: inomhustemperatur: 27°CTT, 19°CVT, utomhustemperatur: 35 °CTT, ekvivalent köldmedierörledning: 5 m, nivåskillnad: 0 m."]
["","","","","(2) - Nominella värmekapaciteter baseras på: inomhustemperatur: 20°CTT, utomhustemperatur: 7 °CTT, 6 °CVT, ekvivalent köldmedierörledning: 5m, nivåskillnad: 0 m.","(2) - Nominella värmekapaciteter baseras på: inomhustemperatur: 20°CTT, utomhustemperatur: 7 °CTT, 6 °CVT, ekvivalent köldmedierörledning: 5m, nivåskillnad: 0 m."]
["","","","","(3) - Se separat ritning för driftsområde","(3) - Se separat ritning för driftsområde"]
["","","","","(4) - Se separata ritningar för elektriska data","(4) - Se separata ritningar för elektriska data"]
["Kylkapacitet","Nom.","","kW","","4.00"]
["Uppvärmningseffekt","Nom.","","kW","","5.20"]
["Nominell verkningsgrad","Årlig energiförbrukning","","kWh","","554"]
["","COP","","","","3.68"]
["","EER köldfaktor","","","","3.61"]
["","Energimärkningsdirektiv","Kyla","","","A"]
["","","Värme","","","A"]