{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":42,"n_cols":7,"rows_kept":42,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXP-M9 / RXP-M"]
[]
[]
[]
[]
["","","","","FTXP20M5V1B9 / RXP20M5V1B","FTXP25M5V1B9 / RXP25M5V1B","FTXP35M5V1B9 / RXP35M5V1B"]
["Utomhusdel","","","","RXP20M5V1B","RXP25M5V1B","RXP35M5V1B"]
["Kylkapacitet","Min.","","kW","","1.3"]
["","Nom.","","kW","","2.50"]
["","Max.","","kW","","3.0"]
["Uppvärmningseffekt","Min.","","kW","","1.30"]
["","Nom.","","kW","","3.00"]
["","Max.","","kW","","4.00"]
["Nominell verkningsgrad","Årlig energiförbrukning","","kWh","","326"]
["","COP","","","","4.36"]
["","EER köldfaktor","","","","3.83"]
["","Energimärkningsdirektiv","Kyla","","","A"]
["","","Värme","","","A"]
["Anm:","","","","(1) - Nominell kylkapacitet baseras på: inomhustemp.: 27°CTT, 19°CVT, utomhustemperatur: 35 °CTT, ekvivalent köldmedierörledning: 5 m, nivåskillnad: 0 m.","(1) - Nominell kylkapacitet baseras på: inomhustemperatur: 27°CTT, 19°CVT, utomhustemperatur: 35 °CTT, ekvivalent köldmedierörledning: 5 m, nivåskillnad: 0 m.","(1) - Nominell kylkapacitet baseras på: inomhustemp.: 27°CTT, 19°CVT, utomhustemperatur: 35 °CTT, ekvivalent köldmedierörledning: 5 m, nivåskillnad: 0 m."]
["","","","","(2) - Nominella värmekapaciteter baseras på: inomhustemperatur: 20°CTT, utomhustemperatur: 7 °CTT, 6 °CVT, ekvivalent köldmedierörledning: 5m, nivåskillnad: 0 m.","(2) - Nominella värmekapaciteter baseras på: inomhustemperatur: 20°CTT, utomhustemperatur: 7 °CTT, 6 °CVT, ekvivalent köldmedierörledning: 5m, nivåskillnad: 0 m.","(2) - Nominella värmekapaciteter baseras på: inomhustemperatur: 20°CTT, utomhustemperatur: 7 °CTT, 6 °CVT, ekvivalent köldmedierörledning: 5m, nivåskillnad: 0 m."]
["","","","","(3) - Se separata ritningar för elektriska data","(3) - Se separata ritningar för elektriska data","(3) - Se separata ritningar för elektriska data"]
["Kylkapacitet","Min.","","kW","1.3","","1.3"]
["","Nom.","","kW","2.00","","3.50"]
["","Max.","","kW","2.6","","4.0"]
["Värmekapacitet","Min.","","kW","1.30","","1.30"]
["","Nom.","","kW","2.50","","4.00"]
["","Max.","","kW","3.50","","4.80"]
["Nominell verkningsgrad","EER köldfaktor","","","4.02","","3.49"]
["","COP","","","4.77","","4.02"]
["","Årlig energiförbrukning","","kWh","249"]
["","Energimärkningsdirektiv","Kyla","","A","","A"]
["","","Värme","","A","","A"]
["Rumskyla","Energieffektivitetsklass","","","A++","","A++"]
["","Kapacitet","Pdesign","kW","2.00","","3.50"]
["","SEER","","","6.79","","6.62"]
["","Årlig energiförbrukning","","kWh/a","103","","186"]
["Rumsvärme (medelklimat)","Energieffektivitetsklass","","","A++","","A++"]
["","Kapacitet","Pdesign","kW","2.20","","2.80"]
["","SCOP/A","","","4.65","","4.64"]
["","Pdh Värmekapacitet vid -10°","","kW","1.99","","2.33"]
["","Årlig energiförbrukning","","kWh/a","662","","845"]
["Intervall för energieffektivitet","","","","A+++ ~ D","","A+++ ~ D"]