{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":85,"n_cols":12,"rows_kept":85,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXS-G"]
[]
[]
[]
[]
["","","","","","FTXS20G2V1B","FTXS25G2V1B","FTXS35G2V1B","FTXS42G2V1B","FTXS50G2V1B","FTXS60GV1B","FTXS71GV1B"]
["Ljudtrycksnivå","Värme","","Hög","dBA","38","39","42","42","44","","46"]
["","","","Tyst drift","dBA","25","25","26","30","31","","34"]
["","","","Låg","dBA","28","28","29","33","34","","37"]
["","Kyla","","Tyst drift","dBA","22","22","23","30","31","","34"]
["","","","Låg","dBA","25","25","26","33","34","","37"]
["","","","Hög","dBA","38","38","42","42","43","","46"]
["","","","Nom.","dBA","33","34","36","38","39","","42"]
["","Kyla","","Nom.","dBA","32","32","34","38","39","","42"]
["Standardtillbehör","Fotokatalytiskt luftreningsfilter med titanapatit","","","","2","2","2","2","2"]
["","Bruksanvisning","","","","1","1","1","1","1","","1"]
["","Installationsanvisning","","","","1","1","1","1","1","","1"]
["","Trådlös fjärrkontroll","","","","1","1","1","1","1","","1"]
["","Batterier","","","","2","2","2","2","2","","2"]
["","Hållare för fjärrkontroll","","","","1","1","1","1","1","","1"]
["","Fästskruvar för inomhusenhet","","","","2","2","2","2","2","","2"]
["","Monteringsplåt","","","","1","1","1","1","1","","1"]
["Styrsystem","Infrared remote control","","","","","","","","","","ARC452A3"]
["Röranslutningar","Vätska","","YD","mm","6.35","6.35","6.35","6.35","6.35","","6.35"]
["","Gas","","YD","mm","9.52","9.52","9.52","9.52","12.70","","15.9"]
["","Kondensvatten","","","","18","18","18","18","18","","18"]
["Ineffekt","Kyla","","Nom.","kW","","","","","","","0.045 (2), 0.045 (3), 0.045 (4)"]
["","Värme","","Nom.","kW","","","","","","","0.060 (2), 0.060 (3), 0.060 (4)"]
["Ljudeffektsnivå","Kyla","","","dBA","54","54","58","58","59","","63"]
["","Värme","","","dBA","54","55","58","58","60","","62"]
["Mått","Enhets-","","Bredd","mm","800","800","800","800","800","","1,050"]
["","","","Djup","mm","215","215","215","215","215","","250"]
["","","","Höjd","mm","295","295","295","295","295","","290"]
["Hölje","Colour","","","","Vit","Vit","Vit","Vit","Vit","","Vit"]
["Vikt","Enhet","","","kg","9","9","10","10","10","","12"]
["Power supply","Phase","","","","1~","1~","1~","1~","1~","","1~"]
["","Frequency","","","Hz","50","50","50","50","50","","50"]
["","Namn","","","","V1","V1","V1","V1","V1","","V1"]
["","Spänning","","","V","220-240","220-240","220-240","220-240","220-240","","220-240"]
["Anm:","","","","","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - SL: Den tysta fläktnivån av luftflödeshastighetsinställningen"]
["","","","","","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 220V"]
["","","","","","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 230V"]
["Fläkt","Luftflödeshastighet","Kyla","Nom.","m³/min","","","","","","16.0"]
["Ljudtrycksnivå","Kyla","","Nom.","dBA","","","","","","41"]
["Fläkt","Luftflödeshastighet","Värme","Nom.","m³/min","","","","","","14.9"]
["Ljudtrycksnivå","Värme","","Nom.","dBA","","","","","","40"]
["Ineffekt","Kyla","","Nom.","kW","","","","","","0.040 (4) (2) (3), 0.040 (4) (2) (3), 0.040 (4) (2) (3)"]
["","Värme","","Nom.","kW","","","","","","0.045 (4) (2) (3), 0.045 (4) (2) (3), 0.045 (4) (2) (3)"]
["Hölje","Färg","","","","","","","","","Vit"]
["Mått","Enhet","","Höjd","mm","","","","","","290"]
["","","","Bredd","mm","","","","","","1050"]
["","","","Djup","mm","","","","","","250"]
["Vikt","Enhet","","","kg","","","","","","12"]
["Fläkt","Luftflödeshastighet","Kyla","Hög","m³/min","","","","","","16.0"]
["","","","Låg","m³/min","","","","","","11.3"]
["","","","Tyst drift","m³/min","","","","","","10.1"]
["","","Värme","Hög","m³/min","","","","","","17.2"]
["","","","Låg","m³/min","","","","","","12.6"]
["","","","Tyst drift","m³/min","","","","","","11.3"]
["Ljudeffektsnivå","Kyla","","","dBA","","","","","","60"]
["","Värme","","","dBA","","","","","","59"]
["Ljudtrycksnivå","Kyla","","Hög","dBA","","","","","","45"]
["","","","Låg","dBA","","","","","","36"]
["","","","Tyst drift","dBA","","","","","","33"]
["","Värme","","Hög","dBA","","","","","","44"]
["","","","Låg","dBA","","","","","","35"]
["","","","Tyst drift","dBA","","","","","","32"]
["Röranslutningar","Vätska","","YD","mm","","","","","","6.35"]
["","Gas","","YD","mm","","","","","","12.7"]
["","Kondensvatten","","","","","","","","","18"]
["Styrsystem","Infraröd fjärrkontroll","","","","","","","","","ARC452A3"]
["Standardtillbehör","Installation manual","","","","","","","","","1"]
["","Wireless remote control","","","","","","","","","1"]
["","Operation manual","","","","","","","","","1"]
["","Batteries","","","","","","","","","2"]
["","Indoor unit fixing screws","","","","","","","","","2"]
["","Mounting plate","","","","","","","","","1"]
["","Remote control holder","","","","","","","","","1"]
["","Titanium apatite photocatalytic air purification filter","","","","","","","","","2"]
["Strömförsörjning","Namn","","","","","","","","","V1"]
["","Fas","","","","","","","","","1~"]
["","Frequency","","","Hz","","","","","","50"]
["","Spänning","","","V","","","","","","220-240"]
["Standardtillbehör","Fotokatalytiskt luftreningsfilter med titanapatit utan ram","","","","","","","","","","2"]
["Anm:","","","","","","","","","","","(4) - 240V"]