{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":53,"n_cols":6,"rows_kept":53,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTA-BW"]
[]
[]
[]
[]
["","","","","","FTXTA30B2V1BW"]
["Ljudtrycksnivå","Värme","","Hög","dBA","41"]
["","","","Medel","dBA","31"]
["","","","Tyst drift","dBA","19"]
["","","","Låg","dBA","24"]
["","Kyla","","Medel","dBA","32"]
["","","","Tyst drift","dBA","20"]
["","","","Låg","dBA","25"]
["","","","Hög","dBA","43"]
["Standardtillbehör","Installationsanvisning","","","","1"]
["","Bruksanvisning","","","","1"]
["","Luftfilter","","","","2"]
["","Infraröd fjärrkontroll","","","","1"]
["","Fjärrkontrollens monteringsplåt","","","","1"]
["","Skruvpåse","","","","1"]
["","Skruvlock","","","","2"]
["","AAA torrbatterier","","","","2"]
["","Allmänna säkerhetsföreskrifter","","","","1"]
["Köldmedium","GWP","","","","675.0"]
["Styrsystem","Kabelansluten fjärrkontroll","","","","BRC073A4"]
["","Infrared remote control","","","","ARC466A59"]
["Piping connections","Vätska","","YD","mm","6.35"]
["","Gas","","YD","mm","9.50"]
["","Drain","","","","18"]
["Ineffekt","Kyla","","Nom.","kW","0.023"]
["","Värme","","Nom.","kW","0.022"]
["Ljudeffektsnivå","Kyla","","","dBA","60"]
["","Värme","","","dBA","60"]
["Mått","Enhet","","Bredd","mm","798"]
["","","","Djup","mm","189"]
["","","","Höjd","mm","295"]
["Hölje","Colour","","","","Vit"]
["Vikt","Enhet","","","kg","11.5"]
["Fläkt","Luftflödeshastighet","Värme","Hög","m³/min","11.5"]
["","","","Låg","m³/min","6.0"]
["","","","Medel","m³/min","8.0"]
["","","","Tyst drift","m³/min","5.1"]
["","","Kyla","Låg","m³/min","5.7"]
["","","","Medel","m³/min","8.3"]
["","","","Hög","m³/min","11.9"]
["","","","Tyst drift","m³/min","4.6"]
["Power supply","Phase","","","","1~"]
["","Frequency","","","Hz","50"]
["","Namn","","","","V1"]
["","Spänning","","","V","220-240"]
["Anm:","","","","","(1) - Kyla: inomhustemperatur. 27 °CTT, 19,0 °CVT, utomhustemperatur. 35 °CTT, 24 °CVT, ekvivalent rörledningslängd: 5 m"]
["","","","","","(2) - Värme: inomhustemperatur. 20 °CTT; utomhustemperatur 7°CTT, 6°CVT; ekvivalent köldmedierörledning: 5m"]
["","","","","","(3) - Se separata ritningar för elektriska data"]