{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":5,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTA-CW / RXTA-C"]
[]
[]
[]
[]
["","","","","FTXTA30C2V1BW / RXTA30C2V1B"]
["Kylkapacitet","Min.","","kW","1.2"]
["","Nom.","","kW","3"]
["","Max.","","kW","4.6"]
["Värmekapacitet","Min.","","kW","0.8"]
["","Nom.","","kW","3.2"]
["","Max.","","kW","7.1"]
["Nominell verkningsgrad","EER köldfaktor","","","4.89"]
["","COP","","","5.01"]
["","Årlig energiförbrukning","","kWh","307"]
["","Energimärkningsdirektiv","Kyla","","A"]
["","","Värme","","A"]
["Rumskyla","Energieffektivitetsklass","","","A+++"]
["","Kapacitet","Pdesign","kW","3"]
["","SEER","","","8.75"]
["","Årlig energiförbrukning","","kWh/a","120"]
["Rumsvärme (medelklimat)","Energieffektivitetsklass","","","A+++"]
["","Kapacitet","Pdesign","kW","3"]
["","SCOP/A","","","5.17"]
["","Pdh Värmekapacitet vid -10°","","kW","3"]
["","Årlig energiförbrukning","","kWh/a","812"]
["Anm:","","","","(1) - Se separata ritningar för elektriska data"]
["","","","","(2) - Se separat ritning för driftsområde"]
["","","","","(3) - Nominell kylkapacitet baseras på: inomhustemp.: 27°CTT, 19°CVT, utomhustemperatur: 35 °CTT, ekvivalent köldmedierörledning: 5 m, nivåskillnad: 0 m."]
["","","","","(4) - Nominella värmekapaciteter baseras på: inomhustemperatur: 20°CTT, utomhustemperatur: 7 °CTT, 6 °CVT, ekvivalent köldmedierörledning: 5m, nivåskillnad: 0 m."]