{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":55,"n_cols":7,"rows_kept":55,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTM-A"]
[]
[]
[]
[]
["","","","","","FTXTM30A2V1B","FTXTM40A2V1B"]
["Ineffekt","Kyla","","Nom.","kW","0.029","0.053"]
["","Värme","","Nom.","kW","0.024","0.06"]
["Hölje","Färg","","","","Vit","Vit"]
["Mått","Enhet","","Höjd","mm","298","298"]
["","","","Bredd","mm","804","997"]
["","","","Djup","mm","252","292"]
["Vikt","Enhet","","","kg","12","15"]
["Fläkt","Luftflödeshastighet","Kyla","Hög","m³/min","13.2","15.1"]
["","","","Medel","m³/min","8.1","9.2"]
["","","","Låg","m³/min","5.6","5.6"]
["","","","Tyst drift","m³/min","4.8","4.8"]
["","","Värme","Hög","m³/min","11.7","17"]
["","","","Medel","m³/min","7.7","10"]
["","","","Låg","m³/min","5.6","6"]
["","","","Tyst drift","m³/min","4.7","5.1"]
["Ljudeffektsnivå","Kyla","","","dBA","60","60"]
["","Värme","","","dBA","59","60"]
["Ljudtrycksnivå","Kyla","","Hög","dBA","45","46"]
["","","","Medel","dBA","33","32"]
["","","","Låg","dBA","25","24"]
["","","","Tyst drift","dBA","21","20"]
["","Värme","","Hög","dBA","43","46"]
["","","","Medel","dBA","31","31"]
["","","","Låg","dBA","22","22"]
["","","","Tyst drift","dBA","19","19"]
["Köldmedium","GWP","","","","675","675"]
["Röranslutningar","Vätska","","YD","mm","6.35","6.35"]
["","Gas","","YD","mm","9.5","9.5"]
["","Kondensvatten","","","","18","18"]
["Styrsystem","Infraröd fjärrkontroll","","","","ARC466A83","ARC466A83"]
["Standardtillbehör","FTXTM30A2V1B","","","","1"]
["","Installation manual","","","","1","1"]
["","Wireless remote control","","","","1","1"]
["","Screw cover","","","","2","2"]
["","AAA dry-cell batteries","","","","2","2"]
["","General safety precautions","","","","1","1"]
["","Operation manual","","","","1","1"]
["","Titanium apatite deodorizing filter","","","","1","1"]
["","Silver particle filter","","","","1","1"]
["","Remote control holder","","","","1","1"]
["","Screw bag","","","","1","1"]
["Strömförsörjning","Namn","","","","V1","V1"]
["","Fas","","","","1~","1~"]
["","Frequency","","","Hz","50","50"]
["","Spänning","","","V","220-240","220-240"]
["Anm:","","","","","(1) - Kyla: inomhustemperatur. 27 °CTT, 19 °CVT; utomhustemperatur 35 °CTT, 24 °CVT, ekvivalent rörledningslängd: 5 m","(1) - Kyla: inomhustemperatur. 27 °CTT, 19 °CVT; utomhustemperatur 35 °CTT, 24 °CVT, ekvivalent rörledningslängd: 5 m"]
["","","","","","(2) - Värme: inomhustemperatur. 20 °CTT; utomhustemperatur 7°CTT, 6°CVT; ekvivalent köldmedierörledning: 5m","(2) - Värme: inomhustemperatur. 20 °CTT; utomhustemperatur 7°CTT, 6°CVT; ekvivalent köldmedierörledning: 5m"]
["","","","","","(3) - Se separata ritningar för elektriska data","(3) - Se separata ritningar för elektriska data"]
["Standardtillbehör","FTXTM40A2V1B","","","","","1"]