{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":20,"n_cols":6,"rows_kept":20,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTM-M / RXTM-N"]
[]
[]
[]
[]
["","","","","FTXTM30M2V1B / RXTM30N2V1B","FTXTM40M2V1B / RXTM40N2V1B"]
["Kylkapacitet","Min.","","kW","0.70","0.70"]
["","Max.","","kW","4.50","5.10"]
["","Nom.","","kW","3.00","4.00"]
["Nominell verkningsgrad","Årlig energiförbrukning","","kWh","366","542"]
["","EER köldfaktor","","","4.10","3.71"]
["","COP","","","5.34","5.37"]
["","Energimärkningsdirektiv","Kyla","","A","A"]
["","","Värme","","A","A"]
["Värmekapacitet","Nom.","","kW","3.20","4.00"]
["","Min.","","kW","0.80","0.80"]
["","Max.","","kW","6.70","7.20"]
["Anm:","","","","(1) - Se separata ritningar för elektriska data","(1) - Se separata ritningar för elektriska data"]
["","","","","(2) - Kyla: T2: inomhustemp. 26,6 °CTT, 19,4 °CVT, utomhustemperatur. 48°CTT [Btu/hr/W]","(2) - Kyla: T2: inomhustemp. 26,6 °CTT, 19,4 °CVT, utomhustemperatur. 48°CTT [Btu/hr/W]"]
["","","","","(3) - Nominella värmekapaciteter baseras på: inomhustemperatur: 20°CTT, utomhustemperatur: 7 °CTT, 6 °CVT, ekvivalent köldmedierörledning: 5m, nivåskillnad: 0 m.","(3) - Nominella värmekapaciteter baseras på: inomhustemperatur: 20°CTT, utomhustemperatur: 7 °CTT, 6 °CVT, ekvivalent köldmedierörledning: 5m, nivåskillnad: 0 m."]