{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":94,"n_cols":7,"rows_kept":94,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTM-R"]
[]
[]
[]
[]
["","","","","","FTXTM30R2V1B","FTXTM40R2V1B"]
["Ljudtrycksnivå","Värme","","Hög","dBA","45.0"]
["","","","Medel","dBA","31.0"]
["","","","Tyst drift","dBA","19.0"]
["","","","Låg","dBA","22.0"]
["","Kyla","","Medel","dBA","33.0"]
["","","","Tyst drift","dBA","21.0"]
["","","","Låg","dBA","25.0"]
["","","","Hög","dBA","45.0"]
["Standardtillbehör","Installationsanvisning","","","","1"]
["","Bruksanvisning","","","","1"]
["","Trådlös fjärrkontroll","","","","1"]
["","AAA torrbatterier","","","","2"]
["","Hållare för fjärrkontroll","","","","1"]
["","Monteringsplåt","","","","1"]
["","Fästskruvar för inomhusenhet","","","","2"]
["","Silverpartikelfilter","","","","1"]
["Styrsystem","Kabelansluten fjärrkontroll","","","","BRC073A1"]
["","Infrared remote control","","","","ARC466A75"]
["Röranslutningar","Vätska","","YD","mm","6.35"]
["","Gas","","YD","mm","9.50"]
["","Kondensvatten","","","","18"]
["Ineffekt","Kyla","","Nom.","kW","0.035"]
["","Värme","","Nom.","kW","0.039"]
["Sound power level","Kyla","","","dBA","60.0"]
["","Värme","","","dBA","61.0"]
["Mått","Enhet","","Bredd","mm","778"]
["","","","Djup","mm","272"]
["","","","Höjd","mm","295"]
["Hölje","Färg","","","","Vit"]
["Vikt","Enhet","","","kg","10.0"]
["Fläkt","Luftflödeshastighet","Värme","Hög","m³/min","12.5"]
["","","","Låg","m³/min","4.9"]
["","","","Medel","m³/min","7.5"]
["","","","Tyst drift","m³/min","4.0"]
["","","Kyla","Låg","m³/min","5.3"]
["","","","Medel","m³/min","7.8"]
["","","","Hög","m³/min","12.2"]
["","","","Tyst drift","m³/min","4.1"]
["Power supply","Fas","","","","1~"]
["","Frequency","","","Hz","50"]
["","Namn","","","","V1"]
["","Spänning","","","V","220-240"]
["Anm:","","","","","(1) - Kyla: inomhustemperatur. 27 °CTT, 19,0 °CVT, utomhustemperatur. 35 °CTT, 24 °CVT, ekvivalent rörledningslängd: 5 m"]
["","","","","","(2) - Värme: inomhustemperatur. 20 °CTT; utomhustemperatur 7°CTT, 6°CVT; ekvivalent köldmedierörledning: 5m"]
["","","","","","(3) - Se separata ritningar för elektriska data"]
["Ineffekt","Kyla","","Nom.","kW","","0.053"]
["","Värme","","Nom.","kW","","0.06"]
["Hölje","Färg","","","","","Vit"]
["Mått","Enhet","","Höjd","mm","","299"]
["","","","Bredd","mm","","998"]
["","","","Djup","mm","","292"]
["Vikt","Enhet","","","kg","","14.5"]
["Fläkt","Luftflödeshastighet","Kyla","Hög","m³/min","","15.4"]
["","","","Medel","m³/min","","9.5"]
["","","","Låg","m³/min","","5.8"]
["","","","Tyst drift","m³/min","","4.6"]
["","","Värme","Hög","m³/min","","17.5"]
["","","","Medel","m³/min","","10.5"]
["","","","Låg","m³/min","","7.1"]
["","","","Tyst drift","m³/min","","5.9"]
["Ljudeffektsnivå","Kyla","","","dBA","","60"]
["","Värme","","","dBA","","61"]
["Ljudtrycksnivå","Kyla","","Hög","dBA","","46"]
["","","","Medel","dBA","","32"]
["","","","Låg","dBA","","24"]
["","","","Tyst drift","dBA","","20"]
["","Värme","","Hög","dBA","","46"]
["","","","Medel","dBA","","31"]
["","","","Låg","dBA","","22"]
["","","","Tyst drift","dBA","","19"]
["Röranslutningar","Vätska","","YD","mm","","6.35"]
["","Gas","","YD","mm","","9.5"]
["","Kondensvatten","","","","","18"]
["Styrsystem","Infrared remote control","","","","","ARC466A75"]
["Styrsystem","Kabelansluten fjärrkontroll","","","","","BRC073A1"]
["Standardtillbehör","Installation manual","","","","","1"]
["","Wireless remote control","","","","","1"]
["","AAA dry-cell batteries","","","","","2"]
["","Operation manual","","","","","1"]
["","Titanium apatite deodorizing filter","","","","","1"]
["","Silver particle filter","","","","","1"]
["","Indoor unit fixing screws","","","","","2"]
["","Mounting plate","","","","","1"]
["","Remote control holder","","","","","1"]
["Strömförsörjning","Namn","","","","","V1"]
["","Fas","","","","","1~"]
["","Frequency","","","Hz","","50"]
["","Spänning","","","V","","220-240"]