{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":83,"n_cols":7,"rows_kept":83,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTP-K"]
[]
[]
[]
[]
["","","","","","FTXTP25K3V1B","FTXTP35K3V1B"]
["Ljudtrycksnivå","Värme","","Hög","dBA","43"]
["","","","Medel","dBA","35"]
["","","","Tyst drift","dBA","21"]
["","","","Låg","dBA","26"]
["","Kyla","","Medel","dBA","35"]
["","","","Tyst drift","dBA","21"]
["","","","Låg","dBA","26"]
["","","","Hög","dBA","43"]
["Standardtillbehör","Installationsanvisning","","","","1"]
["","Bruksanvisning","","","","1"]
["","Trådlös fjärrkontroll","","","","1"]
["","AAA torrbatterier","","","","2"]
["","Hållare för fjärrkontroll","","","","1"]
["","Monteringsplåt","","","","1"]
["","Luftreningsfilter med titanapatit","","","","2"]
["","Fästskruvar för inomhusenhet","","","","2"]
["Styrsystem","Wired remote control","","","","BRC944B2, BRC073A1"]
["","Infrared remote control","","","","ARC480A11"]
["Röranslutningar","Vätska","","YD","mm","6.35"]
["","Gas","","YD","mm","9.50"]
["","Kondensvatten","","","","16 (innerdiameter på anslutningsslang)"]
["Ineffekt","Kyla","","Nom.","kW","0.030"]
["","Värme","","Nom.","kW","0.035"]
["Ljudeffektsnivå","Kyla","","","dBA","58"]
["","Värme","","","dBA","58"]
["Mått","Enhet","","Bredd","mm","770"]
["","","","Djup","mm","225"]
["","","","Höjd","mm","285"]
["Hölje","Färg","","","","Vit"]
["Vikt","Enhet","","","kg","9.0"]
["Power supply","Fas","","","","1~"]
["","Frequency","","","Hz","50"]
["","Namn","","","","V1"]
["","Spänning","","","V","220-240"]
["Anm:","","","","","(1) - Se separata ritningar för elektriska data"]
["Ineffekt","Kyla","","Nom.","kW","","0.03"]
["","Värme","","Nom.","kW","","0.035"]
["Hölje","Färg","","","","","Vit"]
["Mått","Enhet","","Höjd","mm","","285"]
["","","","Bredd","mm","","770"]
["","","","Djup","mm","","225"]
["Vikt","Enhet","","","kg","","9"]
["Fläkt","Luftflödeshastighet","Kyla","Hög","m³/min","","11.4"]
["","","","Medel","m³/min","","8.2"]
["","","","Låg","m³/min","","5.4"]
["","","","Tyst drift","m³/min","","4.3"]
["","","Värme","Hög","m³/min","","10.8"]
["","","","Medel","m³/min","","7.8"]
["","","","Låg","m³/min","","5.8"]
["","","","Tyst drift","m³/min","","4.9"]
["Ljudeffektsnivå","Kyla","","","dBA","","58"]
["","Värme","","","dBA","","58"]
["Ljudtrycksnivå","Kyla","","Hög","dBA","","43"]
["","","","Medel","dBA","","35"]
["","","","Låg","dBA","","26"]
["","","","Tyst drift","dBA","","21"]
["","Värme","","Hög","dBA","","43"]
["","","","Medel","dBA","","35"]
["","","","Låg","dBA","","26"]
["","","","Tyst drift","dBA","","21"]
["Röranslutningar","Vätska","","YD","mm","","6.35"]
["","Gas","","YD","mm","","9.5"]
["","Kondensvatten","","","","","16 (innerdiameter på anslutningsslang)"]
["Styrsystem","Infrared remote control","","","","","ARC480A11"]
["Styrsystem","Kabelansluten fjärrkontroll","","","","","BRC944B2, BRC073A1"]
["Standardtillbehör","Installation manual","","","","","1"]
["","Wireless remote control","","","","","1"]
["","AAA dry-cell batteries","","","","","2"]
["","Operation manual","","","","","1"]
["","Titanium apatite deodorizing filter","","","","","2"]
["","Indoor unit fixing screws","","","","","2"]
["","Mounting plate","","","","","1"]
["","Remote control holder","","","","","1"]
["Strömförsörjning","Namn","","","","","V1"]
["","Fas","","","","","1~"]
["","Frequency","","","Hz","","50"]
["","Spänning","","","V","","220-240"]