{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":8,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXZ-N"]
[]
[]
[]
[]
["","","","","","FTXZ25NV1B","FTXZ35NV1B","FTXZ50NV1B"]
["Ljudtrycksnivå","Värme","","Hög","dBA","39","42","44"]
["","","","Tyst drift","dBA","19","19","24"]
["","","","Låg","dBA","28","29","31"]
["","Kyla","","Tyst drift","dBA","19","19","23"]
["","","","Låg","dBA","26","27","30"]
["","","","Hög","dBA","38","42","47"]
["","","","Nom.","dBA","35","36","38"]
["","Kyla","","Nom.","dBA","33","35","38"]
["Standardtillbehör","Fotokatalytiskt luftrenings- och luktreducerande filter","","","","1","1","1"]
["","Trådlös fjärrkontroll","","","","1","1","1"]
["","Torrbatterier","","","","2","2","2"]
["","Hållare för fjärrkontroll","","","","1","1","1"]
["","Fästskruvar för inomhusenhet","","","","3","3","3"]
["","Monteringsplåt","","","","1","1","1"]
["Styrsystem","Infrared remote control","","","","ARC477A1","ARC477A1","ARC477A1"]
["Piping connections","Vätska","","YD","mm","6.35","6.35","6.35"]
["","Gas","","YD","mm","9.5","9.5","9.5"]
["Effektförbrukning","Kyla","","Nom.","kW","0.030","0.030","0.030"]
["","Värme","","Nom.","kW","0.030","0.030","0.030"]
["Ljudeffektsnivå","Kyla","","","dBA","54","57","60"]
["","Värme","","","dBA","56","57","59"]
["Mått","Enhets-","","Bredd","mm","798","798","798"]
["","","","Djup","mm","372","372","372"]
["","","","Höjd","mm","295","295","295"]
["Hölje","Colour","","","","Vit","Vit","Vit"]
["Vikt","Enhet","","","kg","15","15","15"]
["Fläkt","Luftflödeshastighet","Värme","Hög","m³/min","11.7","13.3","14.4"]
["","","","Låg","m³/min","6.7","6.9","7.7"]
["","","","Tyst drift","m³/min","4.8","4.8","5.9"]
["","","Kyla","Låg","m³/min","5.3","5.6","6.6"]
["","","","Hög","m³/min","10.7","12.1","15.0"]
["","","","Tyst drift","m³/min","4.0","4.0","4.6"]
["","","","Nom.","m³/min","8.6","9.2","10.7"]
["","","Kyla","Nom.","m³/min","7.5","8.4","9.2"]
["Power supply","Fas","","","","1~","1~","1~"]
["","Namn","","","","V1","V1","V1"]
["","Frequency","","","Hz","50","50","50"]
["","Spänning","","","V","220-240","220-240","220-240"]
["Anm:","","","","","(1) - 220V","(1) - 220V","(1) - 220V"]
["","","","","","(2) - 230V","(2) - 230V","(2) - 230V"]
["","","","","","(3) - 240V","(3) - 240V","(3) - 240V"]
["","","","","","(4) - Framsida på värmeväxlare","(4) - Framsida på värmeväxlare","(4) - Framsida på värmeväxlare"]
["","","","","","(5) - Baksida på värmeväxlare","(5) - Baksida på värmeväxlare","(5) - Baksida på värmeväxlare"]