{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":7,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FUA-A / RZA-D"]
[]
[]
[]
[]
["","","","","FUA100AVEB9 / FUA100AVEB9 / RZA200D7Y1B","FUA71AVEB9 / FUA71AVEB9 / FUA71AVEB9 / RZA200D7Y1B","FUA125AVEB9 / FUA125AVEB9 / RZA250D7Y1B (Archived)"]
["Kylkapacitet","Nom.","","kW","19.0 (1)","19.0 (1)"]
["Rumskyla","SEER","","","7.01","7.39"]
["","ηs,c","","%","278","292"]
["","Årlig energiförbrukning","","kWh/a","1,625","1,543"]
["","Kapacitet","Pdesign","kW","19.0","19.0"]
["Rumsvärme (medelklimat)","Kapacitet","Pdesign","kW","11.2","11.2"]
["","SCOP/A","","","4.10","4.15"]
["","Årlig energiförbrukning","","kWh/a","3,825","3,779"]
["","ηs,h","","%","161","163"]
["Uppvärmningseffekt","Nom.","","kW","22.4 (2)","22.4 (2)"]
["Anm:","","","","(1) - Nominell kylkapacitet baseras på: inomhustemperatur: 27°CTT, 19°CVT, utomhustemperatur: 35 °CTT, ekvivalent köldmedierörledning: 5 m, nivåskillnad: 0 m.","(1) - Nominell kylkapacitet baseras på: inomhustemperatur: 27°CTT, 19°CVT, utomhustemperatur: 35 °CTT, ekvivalent köldmedierörledning: 5 m, nivåskillnad: 0 m.","(1) - Nominell kylkapacitet baseras på: inomhustemp.: 27°CTT, 19°CVT, utomhustemperatur: 35 °CTT, ekvivalent köldmedierörledning: 5 m, nivåskillnad: 0 m."]
["","","","","(2) - Nominella värmekapaciteter baseras på: inomhustemperatur: 20°CTT, utomhustemperatur: 7 °CTT, 6 °CVT, ekvivalent köldmedierörledning: 5m, nivåskillnad: 0 m.","(2) - Nominella värmekapaciteter baseras på: inomhustemperatur: 20°CTT, utomhustemperatur: 7 °CTT, 6 °CVT, ekvivalent köldmedierörledning: 5m, nivåskillnad: 0 m.","(2) - Nominella värmekapaciteter baseras på: inomhustemperatur: 20°CTT, utomhustemperatur: 7 °CTT, 6 °CVT, ekvivalent köldmedierörledning: 5m, nivåskillnad: 0 m."]
["Kylkapacitet","Nom.","","kW","","","22.0 (1)"]
["Värmekapacitet","Nom.","","kW","","","24.0 (2)"]
["Rumskyla","Kapacitet","Pdesign","kW","","","22.0"]
["","SEER","","","","","6.10"]
["","Årlig energiförbrukning","","kWh/a","","","2163"]
["Rumsvärme (medelklimat)","Kapacitet","Pdesign","kW","","","12.1"]
["","SCOP/A","","","","","4.10"]
["","Årlig energiförbrukning","","kWh/a","","","4132"]