{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":16,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FUA-A / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FUA100AVEB / RZQG100L8Y1B","FUA125AVEB / RZQG125L8Y1B","FUA71AVEB / FUA71AVEB / RZQG100L8Y1B","FUA71AVEB / FUA71AVEB / RZQG125L8Y1B","FUA100AVEB9 / RZQG100L8Y1B","FUA125AVEB9 / RZQG125L8Y1B","FUA71AVEB9 / FUA71AVEB9 / RZQG100L8Y1B","FUA71AVEB9 / FUA71AVEB9 / RZQG125L8Y1B","FUA71AVEB / RZQG71L8Y1B","FUA100AVEB / RZQG71L8Y1B","FUA100AVEB9 / RZQG71L8Y1B","FUA71AVEB9 / RZQG71L8Y1B"]
["Kylkapacitet","Nom.","","kW","","","","","","","","","6.80","6.80","6.80","6.80"]
["Rumskyla","SEER","","","","","","","","","","","6.42","6.42","6.42","6.42"]
["","Årlig energiförbrukning","","kWh/a","","","","","","","","","371","371","371","371"]
["","Kapacitet","Pdesign","kW","","","","","","","","","6.80","6.80","6.80","6.80"]
["","Energieffektivitetsklass","","","","","","","","","","","A++","A++","A++","A++"]
["Rumsvärme (medelklimat)","Kapacitet","Pdesign","kW","","","","","","","","","7.60","7.60","7.60","7.60"]
["","SCOP/A","","","","","","","","","","","4.20","4.20","4.20","4.20"]
["","Energieffektivitetsklass","","","","","","","","","","","A+","A+","A+","A+"]
["","Årlig energiförbrukning","","kWh/a","","","","","","","","","2,534","2,534","2,534","2,534"]
["Nominell verkningsgrad","Årlig energiförbrukning","","kWh","","","","","","","","","835","","","835"]
["","EER köldfaktor","","","","","","","","","","","4.07","4.07","4.07","4.07"]
["","COP","","","","","","","","","","","4.08","","","4.08"]
["","Energimärkningsdirektiv","Kyla","","","","","","","","","","A","","","A"]
["","","Värme","","","","","","","","","","A","","","A"]
["Uppvärmningseffekt","Nom.","","kW","","","","","","","","","7.50","","","7.50"]
["Anm:","","","","","","","","","","","","(1) - Nominell kylkapacitet baseras på: inomhustemperatur: 27°CTT, 19°CVT, utomhustemperatur: 35 °CTT, ekvivalent köldmedierörledning: 5 m, nivåskillnad: 0 m.","(1) - Se separat ritning för driftsområde","(1) - Se separat ritning för driftsområde","(1) - Nominell kylkapacitet baseras på: inomhustemperatur: 27°CTT, 19°CVT, utomhustemperatur: 35 °CTT, ekvivalent köldmedierörledning: 5 m, nivåskillnad: 0 m."]
["","","","","","","","","","","","","(2) - Nominella värmekapaciteter baseras på: inomhustemperatur: 20°CTT, utomhustemperatur: 7 °CTT, 6 °CVT, ekvivalent köldmedierörledning: 5m, nivåskillnad: 0 m.","(2) - Se separata ritningar för elektriska data","(2) - Se separata ritningar för elektriska data","(2) - Nominella värmekapaciteter baseras på: inomhustemperatur: 20°CTT, utomhustemperatur: 7 °CTT, 6 °CVT, ekvivalent köldmedierörledning: 5m, nivåskillnad: 0 m."]
["","","","","","","","","","","","","(3) - Se separat ritning för driftsområde","","","(3) - Se separat ritning för driftsområde"]
["","","","","","","","","","","","","(4) - Se separata ritningar för elektriska data","","","(4) - Se separata ritningar för elektriska data"]
["Intervall för energieffektivitet","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D"]