{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":18,"n_cols":7,"rows_kept":18,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FUA-A / RZQG-L9V1"]
[]
[]
[]
[]
["","","","","FUA100AVEB9 / RZQG71L9V1B","FUA71AVEB / FUA71AVEB / RZQG125L9V1B","FUA71AVEB9 / FUA71AVEB9 / RZQG125L9V1B"]
["Kylkapacitet","Nom.","","kW","6.80","","12.00"]
["Rumskyla","SEER","","","6.42","5.10","5.10"]
["","Årlig energiförbrukning","","kWh/a","371","824","824"]
["","Kapacitet","Pdesign","kW","6.80","12.0","12.00"]
["","Energieffektivitetsklass","","","A++","A","A"]
["Rumsvärme (medelklimat)","Kapacitet","Pdesign","kW","7.60","12.7","12.71"]
["","SCOP/A","","","4.20","3.80","3.80"]
["","Energieffektivitetsklass","","","A+","A","A"]
["","Årlig energiförbrukning","","kWh/a","2,534","4,683","4,683"]
["Nominell verkningsgrad","EER köldfaktor","","","4.07","","3.61"]
["Anm:","","","","(1) - Se separat ritning för driftsområde","","(1) - Se separat ritning för driftsområde"]
["","","","","(2) - Se separata ritningar för elektriska data","","(2) - Se separata ritningar för elektriska data"]