{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":82,"n_cols":11,"rows_kept":82,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FUA-A"]
[]
[]
[]
[]
["","","","","","FUA71AVEB9","FUA100AVEB9","FUA125AVEB9","FUA71AVEB (Archived)","FUA100AVEB (Archived)","FUA125AVEB (Archived)"]
["Ljudtrycksnivå","Värme","","Hög","dBA","","","","41","46","47"]
["","","","Medel","dBA","","","","38","42","43"]
["","","","Låg","dBA","","","","35","39","40"]
["","Kyla","","Medium","dBA","","","","38","42","43"]
["","","","Låg","dBA","","","","35","39","40"]
["","","","Hög","dBA","","","","41","46","47"]
["Standardtillbehör","Bruksanvisning","","","","","","","1","1","1"]
["","Installationsanvisning","","","","","","","1","1","1"]
["","Kondensvattenslang","","","","","","","1","1","1"]
["","Termiskt isoleringsrör","","","","","","","3","3","3"]
["","Buntband","","","","","","","10","10","10"]
["","Slangband","","","","","","","1","1","1"]
["","Tätningsmaterial","","","","","","","4","4","4"]
["","Brickhållarplåt","","","","","","","1","1","1"]
["","Kondensvattenkoppling","","","","","","","1","1","1"]
["","Ej vävt material","","","","","","","1","1","1"]
["","Bricka","","","","","","","8","8","8"]
["","Fästskruv för kondensvattenslang","","","","","","","5","5","5"]
["Styrsystem","Wired remote control","","","","","","","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52"]
["Kylkapacitet","Total kapacitet","","Nom.","kW","","","","","","12.1"]
["Röranslutningar","Vätska","","YD","mm","","","","9.52","9.52","9.52"]
["","Gas","","YD","mm","","","","15.9","15.9","15.9"]
["","Kondensvatten","","","","","","","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)"]
["Sound power level","Kyla","","","dBA","","","","59","64","65"]
["","Värme","","","dBA","","","","59","64"]
["Mått","Enhet","","Bredd","mm","","","","950","950","950"]
["","","","Djup","mm","","","","950","950","950"]
["","","","Höjd","mm","","","","198","198","198"]
["Hölje","Material","","","","","","","Plast","Plast","Plast"]
["","Färg","","","","","","","Fräscht vit","Fräscht vit","Fräscht vit"]
["Vikt","Enhet","","","kg","","","","25.0","26.0","26"]
["Fläkt","Luftflödeshastighet","Värme","Hög","m³/min","","","","23.0","31.0","32.5"]
["","","","Medium","m³/min","","","","19.5","25.5","26.5"]
["","","","Låg","m³/min","","","","16.0","20.0","20.5"]
["","","Kyla","Låg","m³/min","","","","16.0","20.0","20.5"]
["","","","Medium","m³/min","","","","19.5","25.5","26.5"]
["","","","Hög","m³/min","","","","23.0","31.0","32.5"]
["Dräneringshöjd","mm","","","","","","","600","600","600"]
["Uppvärmningseffekt","Total capacity","","Nom.","kW","","","","","","13.5"]
["Hölje","Färg","","","","Fräscht vit","Fräscht vit","Fräscht vit"]
["","Material","","","","Plast","Plast","Plast"]
["Mått","Enhet","","Höjd","mm","198","198","198"]
["","","","Bredd","mm","950","950","950"]
["","","","Djup","mm","950","950","950"]
["Vikt","Enhet","","","kg","25.0","26.0","26.0"]
["Fläkt","Luftflödeshastighet","Kyla","Hög","m³/min","23.0","31.0","32.5"]
["","","","Medel","m³/min","19.5","25.5","26.5"]
["","","","Låg","m³/min","16.0","20.0","20.5"]
["","","Värme","Hög","m³/min","23.0","31.0","32.5"]
["","","","Medel","m³/min","19.5","25.5","26.5"]
["","","","Låg","m³/min","16.0","20.0","20.5"]
["Ljudeffektsnivå","Kyla","","","dBA","59","64","65"]
["Ljudtrycksnivå","Kyla","","Hög","dBA","41","46","47"]
["","","","Medel","dBA","38","42","43"]
["","","","Låg","dBA","35","39","40"]
["","Värme","","Hög","dBA","41","46","47"]
["","","","Medel","dBA","38","42","43"]
["","","","Låg","dBA","35","39","40"]
["Röranslutningar","Vätska","","YD","mm","9.52","9.52","9.52"]
["","Gas","","YD","mm","15.9","15.9","15.9"]
["","Kondensvatten","","","","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)"]
["Dräneringshöjd","mm","","","","600","600","600"]
["Standardtillbehör","Installation manual","","","","1","1","1"]
["","Thermal insulation tube","","","","3","3","3"]
["","Non woven fabric","","","","1","1","1"]
["","Drain joint","","","","1","1","1"]
["","Hose band","","","","1","1","1"]
["","Operation manual","","","","1","1","1"]
["","Drain hose","","","","1","1","1"]
["","Fixing screw for drain hose","","","","5","5","5"]
["","Sealing material","","","","4","4","4"]
["","Tie-wraps","","","","10","10","10"]
["","Washer","","","","8","8","8"]
["","Washer fixing plate","","","","1","1","1"]
["Kylkapacitet","Total kapacitet","","Nom.","kW","","","12.10"]
["Värmekapacitet","Total kapacitet","","Nom.","kW","","","13.5"]