{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":45,"n_cols":7,"rows_kept":45,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FUQ-C"]
[]
[]
[]
[]
["","","","","FUQ71CVEB","FUQ100CVEB","FUQ125CVEB"]
["Ljudtrycksnivå","Värme","Hög","dBA","41","46","47"]
["","","Nom.","dBA","38","42","43"]
["","","Låg","dBA","35","39","40"]
["","Kyla","Låg","dBA","35","39","40"]
["","","Hög","dBA","41","46","47"]
["","","Nom.","dBA","38","42","43"]
["Standardtillbehör","Installationsanvisning","","","Installationsanvisning","Installationsanvisning","Installationsanvisning"]
["","Bruksanvisning","","","Bruksanvisning","Bruksanvisning","Bruksanvisning"]
["","Konformitetsdeklaration","","","Konformitetsdeklaration","Konformitetsdeklaration","Konformitetsdeklaration"]
["","Kondensvattenslang","","","Kondensvattenslang","Kondensvattenslang","Kondensvattenslang"]
["","Metall för rörhållare","","","Metall för rörhållare","Metall för rörhållare","Metall för rörhållare"]
["","Bricka för hängarfäste","","","Bricka för hängarfäste","Bricka för hängarfäste","Bricka för hängarfäste"]
["","Rörhållare","","","Rörhållare","Rörhållare","Rörhållare"]
["","Brickhållare","","","Brickhållare","Brickhållare","Brickhållare"]
["","Kopplingsisolerings- och tätningsmaterial","","","Kopplingsisolerings- och tätningsmaterial","Kopplingsisolerings- och tätningsmaterial","Kopplingsisolerings- och tätningsmaterial"]
["","Vinkel","","","Vinkel","Vinkel","Vinkel"]
["","Installationsmönster","","","Installationsmönster","Installationsmönster","Installationsmönster"]
["","Blockeringsmaterial","","","Blockeringsmaterial","Blockeringsmaterial","Blockeringsmaterial"]
["","Rör med L-böj","","","Rör med L-böj","Rör med L-böj","Rör med L-böj"]
["","Skruvar","","","Skruvar","Skruvar","Skruvar"]
["","Ej vävt material","","","Ej vävt material","Ej vävt material","Ej vävt material"]
["Styrsystem","Kabelansluten fjärrkontroll","","","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B"]
["","Infrared remote control","","","BRC7C58","BRC7C58","BRC7C58"]
["Röranslutningar","Vätska","YD","mm","9.52","9.52","9.52"]
["","Gas","YD","mm","15.9","15.9","15.9"]
["","Kondensvatten","","","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)"]
["Sound power level","Kyla","","dBA","59","64","65"]
["","Värme","","dBA","59","64","65"]
["Mått","Enhet","Bredd","mm","950","950","950"]
["","","Djup","mm","950","950","950"]
["","","Höjd","mm","198","198","198"]
["Hölje","Material","","","Plast","Plast","Plast"]
["","Färg","","","Fräscht vit","Fräscht vit","Fräscht vit"]
["Vikt","Enhet","","kg","25","26","26"]
["Dräneringshöjd","mm","","","600","600","600"]
["Power supply","Fas","","","1~","1~","1~"]
["","Frequency","","Hz","50/60","50/60","50/60"]
["","Namn","","","VE","VE","VE"]
["","Spänning","","V","220-240/220","220-240/220","220-240/220"]