{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":11,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVQ-C / RZQG-L9V1"]
[]
[]
[]
[]
["","","","","FVQ100CVEB / RZQG71L9V1B","FVQ71CVEB / RZQG71L9V1B","FVQ100CVEB / RZQG100L9V1B","FVQ140CVEB / RZQG100L9V1B","FVQ140CVEB / RZQG125L9V1B","FVQ125CVEB / RZQG125L9V1B","FVQ140CVEB / RZQG140L9V1B"]
["Kylkapacitet","Nom.","","kW","","6.8","9.5","","","12.0","13.4"]
["Rumskyla","SEER","","","6.31","6.23","5.61","5.61","5.61","5.61"]
["","Årlig energiförbrukning","","kWh/a","378","383","593","593","749","749"]
["","Kapacitet","Pdesign","kW","6.80","6.80","9.50","9.50","12.00","12.00"]
["","Energieffektivitetsklass","","","A++","A++","A+","A+","A+","A+"]
["Rumsvärme (medelklimat)","Kapacitet","Pdesign","kW","6.33","6.33","11.30","11.30","11.30","11.30"]
["","SCOP/A","","","4.05","4.05","4.20","4.20","3.87","3.87"]
["","Energieffektivitetsklass","","","A+","A+","A+","A+","A","A"]
["","Årlig energiförbrukning","","kWh/a","2,189","2,189","3,767","3,767","4,088","4,088"]
["Nominell verkningsgrad","Årlig energiförbrukning","","kWh","","1,010","1,245","","","1,870","2,085"]
["","EER köldfaktor","","","","3.37","3.81","","","3.21","3.21"]
["","COP","","","","3.64","4.14","","","3.70","3.61"]
["","Energimärkningsdirektiv","Kyla","","","A","A","","","A"]
["","","Värme","","","A","A","","","A"]
["Uppvärmningseffekt","Nom.","","kW","","7.5","10.8","","","13.5","15.5"]
["Anm:","","","","","(1) - Årlig energiförbruking enligt Energimärkningsdirektiv 2002/31/EC","(1) - EER/COP enligt Eurovent 2012, endast för användning utanför EU","","","(1) - EER/COP enligt Eurovent 2012, endast för användning utanför EU","(1) - EER/COP enligt Eurovent 2012, endast för användning utanför EU"]
["","","","","","(2) - SEER och SCOP är enligt EN 14825","(2) - Nominell verkningsgrad: kyla vid 35°/27° nominell last, värme vid 7°/20° nominell last","","","(2) - Nominell verkningsgrad: kyla vid 35°/27° nominell last, värme vid 7°/20° nominell last","(2) - Nominell verkningsgrad: kyla vid 35°/27° nominell last, värme vid 7°/20° nominell last"]