{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":8,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVXM-A / RXTP-N8"]
[]
[]
[]
[]
["","","","","FVXM25A2V1B / RXTP25N2V1B8","FVXM25A3V1B / RXTP25N2V1B8","FVXM35A2V1B / RXTP35N2V1B8","FVXM35A3V1B / RXTP35N2V1B8"]
["Kylkapacitet","Min.","","kW","1.40","","1.40"]
["","Max.","","kW","4.20","","4.30"]
["","Nom.","","kW","2.50","","3.50"]
["Nominell verkningsgrad","Årlig energiförbrukning","","kWh","328","","510"]
["","EER köldfaktor","","","3.81","","3.43"]
["","COP","","","3.86","","3.54"]
["","Energimärkningsdirektiv","Kyla","","A","","A"]
["","","Värme","","A","","B"]
["Uppvärmningseffekt","Nom.","","kW","3.20","","4.00"]
["","Min.","","kW","1.20","","1.20"]
["","Max.","","kW","5.70","","6.20"]
["Anm:","","","","(1) - Nominell kylkapacitet baseras på: inomhustemperatur: 27°CTT, 19°CVT, utomhustemperatur: 35 °CTT, ekvivalent köldmedierörledning: 5 m, nivåskillnad: 0 m.","","(1) - Nominell kylkapacitet baseras på: inomhustemperatur: 27°CTT, 19°CVT, utomhustemperatur: 35 °CTT, ekvivalent köldmedierörledning: 5 m, nivåskillnad: 0 m."]
["","","","","(2) - Nominella värmekapaciteter baseras på: inomhustemperatur: 20°CTT, utomhustemperatur: 7 °CTT, 6 °CVT, ekvivalent köldmedierörledning: 5m, nivåskillnad: 0 m.","","(2) - Nominella värmekapaciteter baseras på: inomhustemperatur: 20°CTT, utomhustemperatur: 7 °CTT, 6 °CVT, ekvivalent köldmedierörledning: 5m, nivåskillnad: 0 m."]
["","","","","(3) - Se separata ritningar för elektriska data","","(3) - Se separata ritningar för elektriska data"]
["","","","","(4) - Se separat ritning för driftsområde","","(4) - Se separat ritning för driftsområde"]
["Kylkapacitet","Min.","","kW","","1.00","","1.10"]
["","Nom.","","kW","","2.50","","3.50"]
["","Max.","","kW","","4.20","","4.30"]
["Värmekapacitet","Min.","","kW","","1.00","","1.10"]
["","Nom.","","kW","","3.20","","4.00"]
["","Max.","","kW","","5.70","","6.20"]
["Nominell verkningsgrad","EER köldfaktor","","","","3.81","","3.43"]
["","COP","","","","3.86","","3.54"]
["","Årlig energiförbrukning","","kWh","","328","","510"]
["","Energimärkningsdirektiv","Kyla","","","A","","A"]
["","","Värme","","","A","","B"]
["Rumskyla","Energieffektivitetsklass","","","","A++","","A++"]
["","Kapacitet","Pdesign","kW","","2.50","","3.50"]
["","SEER","","","","6.50","","6.10"]
["","Årlig energiförbrukning","","kWh/a","","135","","201"]
["Rumsvärme (medelklimat)","Energieffektivitetsklass","","","","A++","","A++"]
["","Kapacitet","Pdesign","kW","","2.50","","3.00"]
["","SCOP/A","","","","4.70","","4.60"]
["","Pdh Värmekapacitet vid -10°","","kW","","2.50","","3.00"]
["","Årlig energiförbrukning","","kWh/a","","744","","913"]