{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":52,"n_cols":6,"rows_kept":52,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVXTM-B"]
[]
[]
[]
[]
["","","","","","FVXTM30B2V1B"]
["Ineffekt","Kyla","","Nom.","kW","0.02"]
["","Värme","","Nom.","kW","0.03"]
["Hölje","Färg","","","","Vit"]
["Mått","Enhet","","Höjd","mm","600"]
["","","","Bredd","mm","750"]
["","","","Djup","mm","238"]
["Vikt","Enhet","","","kg","17"]
["Fläkt","Luftflödeshastighet","Kyla","Hög","m³/min","9"]
["","","","Medel","m³/min","6.7"]
["","","","Låg","m³/min","4.8"]
["","","","Tyst drift","m³/min","4"]
["","","Värme","Hög","m³/min","9.4"]
["","","","Medel","m³/min","6.8"]
["","","","Låg","m³/min","5.3"]
["","","","Tyst drift","m³/min","4"]
["Ljudeffektsnivå","Kyla","","","dBA","53"]
["","Värme","","","dBA","53"]
["Ljudtrycksnivå","Kyla","","Hög","dBA","39"]
["","","","Medel","dBA","32"]
["","","","Låg","dBA","25"]
["","","","Tyst drift","dBA","20"]
["","Värme","","Hög","dBA","39"]
["","","","Medel","dBA","32"]
["","","","Låg","dBA","25"]
["","","","Tyst drift","dBA","19"]
["Köldmedium","GWP","","","","675"]
["Röranslutningar","Vätska","","YD","mm","6.35"]
["","Gas","","YD","mm","9.5"]
["","Kondensvatten","","","","VP20 (I.D. 20/O.D. 26)"]
["Styrsystem","Infraröd fjärrkontroll","","","","ARC466A90"]
["","Kabelansluten fjärrkontroll","","","","BRC073A1"]
["Standardtillbehör","Installation manual","","","","1"]
["","Wireless remote control","","","","1"]
["","AAA dry-cell batteries","","","","2"]
["","General safety precautions","","","","1"]
["","Operation manual","","","","1"]
["","Titanium apatite deodorizing filter","","","","2"]
["","Remote control holder","","","","1"]
["","Screw bag","","","","1"]
["Strömförsörjning","Namn","","","","V1"]
["","Fas","","","","1~"]
["","Frequency","","","Hz","50"]
["","Spänning","","","V","220-240"]
["Anm:","","","","","(1) - Kyla: inomhustemperatur. 27 °CTT, 19 °CVT; utomhustemperatur 35 °CTT, 24 °CVT, ekvivalent rörledningslängd: 5 m"]
["","","","","","(2) - Värme: inomhustemperatur. 20 °CTT; utomhustemperatur 7°CTT, 6°CVT; ekvivalent köldmedierörledning: 5m"]
["","","","","","(3) - Se separata ritningar för elektriska data"]